
ANDY DU

SUMMARY
Andy Du is an inspection professional with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has worked across pressure vessels, FPSO packages, subsea products, steel structures, pipes and tubes, fittings, valves, chains, bridges, and heavy lifting equipment. His experience includes resident and mechanical inspection, coating inspection, vendor and manufacturer surveillance, document review, welding-process monitoring, NDT witnessing, dimensional and visual inspection, testing, final inspection, and packing review. Andy has broad knowledge of international and national standards and welding processes including SAW, SMAW, GTAW, FCAW, and GMAW. He has coordinated effectively between contractors and clients on large projects.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed resident, mechanical, material, third-party, welding, coating, pressure vessel, FPSO package, subsea product, steel structure, crane, bridge, and equipment inspection across major fabrication and energy projects.
Monitored fabrication, welding, NDT, coating, testing, dimensional and visual quality, assembly, FAT, final inspection, packing, shipping, and preservation.
Reviewed MTRs, quality-control documents, ITPs, WPS/PQRs, WQT records, certificates, MRBs, procedures, and manufacturing documentation.
Coordinated inspection activities between contractors, manufacturers, clients, suppliers, and end users.

PROJECTS

Client: TEN (End user Total)
GRANMOR PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Inspected marking and openings, nozzle fit-up and welding to shells and heads, NDT, internal cleaning, visual and dimensional requirements.
Witnessed hydrostatic and weighing tests and inspected pickling, passivation, painting, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection of flanges, elbows, and forgings.
Monitored clad welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Performed visual and clad-thickness inspection, witnessed NDT and PMI testing, and reviewed documents.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection, and inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Inspected marking and openings, nozzle fit-up and welding to shells and heads, NDT, internal cleaning, visual and dimensional requirements.
Witnessed hydrostatic and weighing tests and inspected pickling, passivation, painting, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection, and inspected formed heads.
Inspected fit-up and tack welding, marking and openings, nozzle fit-up and welding to shells and heads.
Witnessed chemical analysis of cladding, NDT, hydrostatic and weighing tests.
Inspected internal cleaning, visual and dimensional requirements, pickling, passivation, nameplates, marking, packing, and reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection, and inspected formed heads.
Inspected fit-up and tack welding, monitored welding processes, marking and openings, and nozzle fit-up and welding to shells and heads.
Performed PWHT inspection and witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional requirements, pickling, passivation, nameplates, weighing, marking, packing, and reviewed MRB documentation.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection, and inspected formed heads, fit-up, tack welding, marking, and openings.
Monitored welding to WPS and PQR requirements for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected nozzle fit-up and welding to shells and heads, PWHT, NDT, internal cleaning, and visual and dimensional requirements.
Witnessed air-tight leak and hydrostatic tests and inspected pickling, passivation, blasting, painting, nameplates, final inspection, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material inspection, MTR review, receipt inspection, head forming, material cutting, and traceability.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding to WPS and PQR requirements.
Inspected marking, openings, nozzle fit-up and welding to shells and heads, PWHT, NDT, internal cleaning, and visual and dimensional requirements.
Witnessed PMI, hardness, air-tight leak, hydrostatic, and weighing tests.
Inspected pickling, passivation, nameplates, marking, packing, and reviewed MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material inspection, MTR review, receipt inspection, head forming, material cutting, and traceability.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding to WPS and PQR requirements.
Inspected marking, openings, nozzle fit-up and welding to shells and heads, PWHT, NDT, internal cleaning, and visual and dimensional requirements.
Witnessed PMI, hardness, air-tight leak, hydrostatic, and weighing tests.
Inspected pickling, passivation, nameplates, marking, packing, and reviewed MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material and head-forming inspection and inspected fit-up, tack welding, marking, openings, and nozzle fit-up and welding to shells and heads.
Monitored welding processes and performed visual and dimensional inspection after welding.
Performed heat-treatment and hydrostatic-test inspection.
Inspected blasting and painting, final inspection, package shipping, preservation, and reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic testing and performed cleanliness and final inspection.
Inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic and helium/nitrogen leakage testing.
Performed final inspection and inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Performed dimensional and visual inspection, hydrostatic testing, blasting and painting inspection, and flange management inspection.
Monitored structure, piping spool, valve, and other free-issue installation and performed mechanical completion checks.
Witnessed FAT and performed final inspection, package shipping, and preservation inspection.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspection
Monitored feed gas heater and membrane housing fabrication.
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional and visual inspection.
Inspected blasting, painting, insulation, flange management, mechanical completion, FAT, final inspection, and package shipping and preservation.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional and visual inspection.
Inspected blasting, painting, insulation, flange management, and mechanical completion.
Witnessed FAT, system leak testing, weighing and COG inspection, final inspection, package shipping, and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings and performed vessel fabrication inspection.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, insulation, flange management, and mechanical completion.
Witnessed FAT, system leak testing, weighing and COG inspection, and final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, insulation, flange management, and mechanical completion.
Witnessed FAT, system leak testing, weighing and COG inspection, final inspection, package shipping, and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, insulation, flange management, and mechanical completion.
Witnessed FAT, system leak testing, weighing and COG inspection, final inspection, package shipping, and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, insulation, flange management, and mechanical completion.
Witnessed FAT, system leak testing, weighing and COG inspection, final inspection, package shipping, and preservation.

Client: PSA CORPORATION LTD and other stated clients
Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspection
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Performed parts machining quality, fit-up, and welding inspection.
Witnessed function, vibration, and noise tests and inspected package shipping and preservation.
Reviewed documents.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.
Performed CPT testing.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents and coating-system qualification.
Inspected paint and coating materials, surface cleanliness, abrasive and compressed air, environmental conditions, and blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed documents.
Performed visual examination and DFT inspection, paint repair inspection, and adhesion inspection by pull-off and crosscut testing.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents and inspected pickling, passivation, and coating-system qualification.
Inspected paint and coating materials, surface cleanliness, abrasive and compressed air, environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface cleanliness, environmental conditions, abrasive and compressed air, and blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual examination, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Client: Jiangnan Boiler & Pressure Vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler & Pressure Vessel
Position: NACE CIP coating inspector
Reviewed documents and inspected cleanliness after blasting, including cleanliness, roughness, and dust.
Inspected curing, visual examination and DFT for each layer, paint repairs, crosscut adhesion, and final and marking inspection.

Client: Baker Hughes
XT system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Tree frame, protection structure, debris cap, debris canopy, shipping skid
Position: Inspector
Performed raw material inspection, including MTR review and receipt inspection, material cutting and marking, machining, fit-up, and structural welding monitoring.
Witnessed UT and MT of welds and performed visual weld inspection and base-frame dimensional verification.
Inspected coating surface preparation, painting, adhesion, holiday testing, assembly, FAT, final inspection, MRB, package, and shipping.

Client: Baker Hughes
Connections system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Clamp connectors (VCCS & HCCS Type T, HCCS-L, Test Clamp), Pressure Caps, Vent caps, Light Duty Clamps
Position: Inspector
Performed raw material and machining inspection and NDT inspection before clad welding.
Monitored clad welding and inspected PMI, CRA thickness, NDT, hardness, dimensions, load testing, blasting, painting, assembly, and adhesion and holiday testing.
Witnessed FAT including weight, visual, electrical continuity, and COG testing.
Performed final, MRB, package, and shipping inspection.

Client: Baker Hughes
GFDS System
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Porch, Termination, Male Hub/pup-piece
Position: Inspector
Performed raw material and machining inspection and NDT inspection before clad welding.
Monitored clad welding and inspected PMI, CRA thickness, NDT, dimensions, blasting, painting, and assembly.
Witnessed hydrostatic, gas, adhesion, holiday, and FAT testing, including weight, visual, electrical continuity, and back-seal testing.
Performed final, MRB, package, and shipping inspection.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Third party inspection & Certification of Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Position: Third party inspector
Performed manufacturing procedure qualification testing and product chemical analysis and mechanical property testing.
Witnessed hydrostatic and NDT testing, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection and inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Standards: ASME B16.5, ASME B16.9, ASME B16.11, MSS SP-97
Position: Third party inspector
Reviewed documents and witnessed chemical analysis, mechanical property, hardness, and PMI testing.
Performed dimensional and visual quality inspection and inspected packing, marking, and coating.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Position: Third party inspector
Reviewed documents and witnessed PMI, mechanical property, hardness, and NDT testing including PT, MT, UT, and RT.
Performed assembly, visual, and dimensional inspection.
Witnessed hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Standards: API 14A, API 11D
Position: Third party inspector
Reviewed documents and witnessed drift and function testing.
Performed dimensional, visual, marking, coating, and protection inspection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Position: Third party inspector
Reviewed documents and witnessed chemical analysis and mechanical property testing.
Performed hardness, UT, MT, visual, and dimensional inspection.
Inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspector
Reviewed documents and witnessed chemical analysis and mechanical property testing.
Witnessed proof-load and break-load testing.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Position: Third party inspector
Reviewed documents and monitored casing.
Performed chemical and electrochemical analysis, cross-cut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Position: Third party inspector
Reviewed documents and witnessed hydrostatic, performance, and break-load testing.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Container
Position: Inspector
Reviewed documents and performed floorboard and corner-fitting sampling.
Witnessed relative testing and inspected welding processes, assembly, dimensions, and visual quality after welding.
Performed coating inspection, witnessed general prototype testing, and completed whole-container inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Position: Inspector
Reviewed related documents and procedures, including WPS, welder qualifications, and drawings.
Performed raw material re-inspection and inspected main structural steel assembly.
Inspected pre-welding and welding processes, visual quality after welding, structural final inspection, and coating.
Witnessed FAT and EFAT of cranes.

Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Product: Steel bridge
Position: CWI inspector
Performed raw material re-inspection and witnessed mechanical property testing and product chemical analysis for steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding and welding processes, visual quality after welding, and zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland Condenser & Handing Clamp
Position: Inspector
Reviewed quality-control documents including ITP, WPS/PQR, WQT, and NDT records.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing and cleaning and dry checks.
Witnessed surface preparation and performed visual and dry-film checks.
Inspected rust prevention, including application of VCI inside the gland condenser.
Performed visual and dimensional inspection including nameplates, packing and marking inspection, and reviewed manufacturing final inspection.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Third-Party Inspection
Mechanical Inspection
Welding Inspection
Coating / Painting Inspection
NDT Inspection
Vendor Surveillance
Pressure Vessel Inspection
FPSO and Package Inspection
Subsea Product Inspection
Steel Structure Inspection
Piping and Valve Inspection
Crane and Heavy Lifting Equipment Inspection
Document Review
Quality Control Document Review
Fabrication Monitoring
Client and Contractor Coordination

COMMODITIES
Coating Material
Pressure Vessels
FPSO Packages
Subsea Structures
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridges
Steel Plates
Forgings
Gas Turbine Cylinders
Skids
Heat Exchangers
Separators
Scrubbers
Pumps
Cranes
Containers
Anodes
Ropes
Buoys
Dynamic Equipment
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