
ANDY DU

SUMMARY
Andy Du is an inspection professional with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has extensive experience inspecting pressure vessels, FPSO and gas-treatment packages, skids, gas turbine cylinders, dynamic equipment, steel structures, bridges, cranes, piping, valves, and subsea products for major international projects and clients including Total, Veolia, SLB, Modec, CNOOC, Air Liquide, and Baker Hughes. His coating inspection scope includes surface preparation, environmental conditions, blasting, paint application, DFT, curing, repair, adhesion, and coating-system qualification. Andy has broad knowledge of international and national standards and welding processes including SAW, SMAW, GTAW, FCAW, and GMAW, together with strong contractor-client coordination capability.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS, ASME, ASTM, API, GB, HB, JB, EN, ISO…

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed material, mechanical, welding, coating, NDT, dimensional, visual, pressure, functional, and document inspection across pressure vessels, packages, skids, subsea products, piping, valves, steel structures, cranes, bridges, and other equipment.
Performed third-party inspection and certification for pipes, tubes, fittings, valves, safety valves, packers, steel plates, forgings, chains, anodes, ropes, and related products.
Coordinated inspection activities between contractors, manufacturers, suppliers, and clients on major international projects.

PROJECTS

Client: TEN (End user Total)
GRANMORU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Witnessed NDT and hydrostatic testing and performed internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, painting, nameplates, weighing, marking, and packing.
Reviewed MRB documentation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection of flanges, elbows, and forgings.
Monitored clad welding processes, including preheat, consumables, welding parameters, welder qualification, and protection.
Performed visual and clad-thickness inspection.
Witnessed NDT and PMI testing.
Performed document review.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection.
Inspected formed heads, fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Witnessed NDT and hydrostatic testing and performed internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, painting, nameplates, weighing, marking, and packing.
Reviewed MRB documentation.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material and formed-head inspection.
Inspected fit-up and tack welding, marking, openings, nozzle fit-up, and welding to shells and heads.
Performed chemical analysis of cladding and witnessed NDT.
Performed internal cleaning, visual, and dimensional inspection and witnessed hydrostatic testing.
Inspected pickling and passivation, nameplates, weighing, marking, and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material and formed-head inspection.
Inspected fit-up and tack welding and monitored the welding process.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Performed PWHT inspection and witnessed NDT and hydrostatic testing.
Performed internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, nameplates, weighing, marking, packing, and MRB documentation.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material and formed-head inspection and inspected fit-up and tack welding.
Monitored welding as per WPS and PQR using GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Performed PWHT inspection and witnessed NDT, air-tight leak testing, and hydrostatic testing.
Performed internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, blasting and painting, nameplates, final inspection, marking, packing, and MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material inspection, formed-head inspection, material cutting, and traceability inspection.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding per WPS and PQR.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Witnessed PMI, hardness testing, NDT, air-tight leak testing, and hydrostatic testing.
Performed PWHT, internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, nameplates, weighing, marking, packing, and MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material inspection, formed-head inspection, material cutting, and traceability inspection.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding per WPS and PQR.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Witnessed PMI, hardness testing, NDT, air-tight leak testing, and hydrostatic testing.
Performed PWHT, internal cleaning, visual, and dimensional inspection.
Inspected pickling and passivation, nameplates, weighing, marking, packing, and MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material and formed-head inspection and inspected fit-up and tack welding.
Monitored welding processes and performed post-weld visual inspection.
Inspected marking, openings, nozzle fit-up, welding to shells and heads, and dimensions.
Performed heat-treatment, hydrostatic, blasting, painting, and final inspection.
Inspected package shipping and preservation and reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic testing and performed cleanliness inspection.
Performed final inspection and inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic testing and helium/nitrogen leakage testing.
Performed final inspection and inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, lifting lugs, piping spool fabrication, and installation.
Performed dimensional and visual inspection, hydrostatic testing, blasting and painting inspection, and flange management inspection.
Performed mechanical completion checks and witnessed FAT.
Performed final inspection and inspected package shipping and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspection
Monitored feed gas heater and membrane housing fabrication.
Inspected raw materials, structure, piping, valves, and pipe fittings.
Monitored primary and secondary structures, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional and visual inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, insulation, and FAT.
Performed final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional and visual inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, and insulation.
Witnessed FAT, system leak testing, weighing and COG inspection.
Performed final inspection and inspected package shipping and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings and performed vessel fabrication inspection.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, and insulation.
Witnessed FAT, system leak testing, weighing and COG inspection and performed final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, and insulation.
Witnessed FAT, system leak testing, weighing and COG inspection.
Performed final inspection and inspected package shipping and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, and insulation.
Witnessed FAT, system leak testing, weighing and COG inspection.
Performed final inspection and inspected package shipping and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspection
Inspected raw materials including structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing and performed dimensional inspection.
Inspected blasting, painting, installation, flange management, mechanical completion, and insulation.
Witnessed FAT, system leak testing, weighing and COG inspection.
Performed final inspection and inspected package shipping and preservation.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspection
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Performed parts machining quality, fit-up, and welding inspection.
Witnessed function, vibration, and noise testing.
Inspected package shipping and preservation and performed document review.

Client: Himile Mechanical Manufacturing Co. Ltd.
Subsea product for Baker Hughes
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: XT system, connection system, and GFDS system products
Inspected XT system tree frames, protection structures, debris caps, debris canopies, and shipping skids.
Inspected connection-system clamp connectors, pressure caps, vent caps, and light-duty clamps.
Inspected GFDS system porches, terminations, male hubs, and pup-pieces.
Performed raw material, machining, material cutting, marking, fit-up, welding, dimensional, visual, coating, assembly, FAT, final, MRB, and package-shipping inspection.
Witnessed UT and MT of welds, PMI, CRA thickness, hardness, load, hydrostatic, gas, adhesion, holiday, electrical continuity, back-seal, weight, and COG tests.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Third party inspection and certification of Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS and welded pipes, 5D inducted bends, stainless steel SMLS and welded tubes, nickel alloy pipes, square and rectangular tube, Cu alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Performed manufacturing procedure qualification testing and chemical and mechanical property testing.
Witnessed hydrostatic and NDT testing, including ET, UT, RT, and MT.
Performed dimensional, visual quality, packing, marking, and coating inspection.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Third party inspection of Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM blind flange, flange, reducer, tee, elbow, weldolet, coupling, thread end cap, sockolet, nipple, and other fittings
Standards: ASME B16.5, ASME B16.9, ASME B16.11, MSS SP-97
Performed document review, chemical analysis, mechanical property, hardness, and PMI testing.
Performed dimensional, visual quality, packing, marking, and coating inspection.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Third party inspection of Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Performed document review, PMI, mechanical property, and hardness testing.
Witnessed PT, MT, UT, and RT NDT and performed assembly, visual, and dimensional inspection.
Witnessed hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
Third party inspection of SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Product: SubSurface Safety Valve and Packer
Standards: API 14A, API 11D
Reviewed documents and witnessed drift and function testing.
Performed dimensional, visual, marking, coating, and protection inspection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Third party inspection of Steel plates and forging
Product: Shipped steel plates, spheroidal graphite cast iron, AISI 4130 and 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Performed document review, chemical analysis, mechanical property, and hardness testing.
Witnessed UT and MT and performed visual, dimensional, painting, marking, and packing inspection.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Third party inspection of Chain
Product: Mooring chain cable, wire rope sling, Tonsberg mooring links, Mandal fairlead shackle, chain grapnel, J hook, and pear links
Performed document review, chemical analysis, and mechanical property testing.
Witnessed proof-load and break-load testing.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Third party inspection of Anodes
Product: Al Anode, Zn Anode
Performed document review and monitored casing.
Performed chemical and electrochemical analysis, cross-cut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Third party inspection of Other products
Product: Electric heater core, life raft, pick-up buoys, anchor buoys, polyamide (Nylone) 8-strand ropes
Performed document review and witnessed hydrostatic, performance, and break-load testing.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC (Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Containers
Reviewed documents and performed floorboard and corner-fitting sampling.
Witnessed relative testing and performed routing inspection covering welding, assembly, and dimensions.
Performed post-welding visual quality, coating, general prototype, and whole-container inspection.

Client: NP QHG port, PSA Corporation Ltd, MEPT, Voltritermianal Europa S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA Panama International, Terminal S.A (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container cranes (RTG/STS), offshore crane, hydraulic slewing crane
Reviewed related documents and procedures, including WPS, welder qualification, and drawings.
Performed raw material re-inspection and inspected main structural steel assembly.
Inspected pre-welding, welding processes, post-welding visual quality, and final structure.
Performed coating inspection and witnessed FAT and EFAT of cranes.

Experience in the construction of bridges
Product: Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Position: CWI inspector
Performed raw material re-inspection and mechanical property and product chemical analysis of steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding, welding processes, post-welding visual quality, and zinc coating of fabricated products.

Client: Samsung Engineering Co., Ltd, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland Condenser and Handing Clamp
Reviewed quality-control documents including ITP, WPS/PQR, WQT, and NDT records.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing and cleaning and dry checks.
Witnessed surface preparation and performed visual and dry-film checks.
Inspected rust prevention, visual and dimensional characteristics, nameplates, packing, and marking.
Reviewed manufacturing final inspection certificates.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed documents and paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet-film thickness, curing, DFT, repairs, and adhesion.
Witnessed CPT testing and performed pull-off and cross-cut adhesion testing.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed documents and paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet-film thickness, curing, DFT, repairs, and adhesion.
Performed pull-off and cross-cut adhesion testing.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Product: Seawater Filter Package
Position: NACE CIP Coating inspector
Reviewed documents and coating-system qualification and paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet-film thickness, curing, DFT, repairs, and adhesion.
Performed pull-off and cross-cut adhesion testing.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed documents.
Performed visual and DFT inspection, paint-repair inspection, and pull-off and cross-cut adhesion testing.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents and performed pickling and passivation inspection.
Inspected coating-system qualification, paint and coating materials, surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet-film thickness, curing, DFT, repairs, and adhesion.
Performed pull-off and cross-cut adhesion testing.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents and paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet-film thickness, curing, DFT, repairs, and adhesion.
Performed pull-off and cross-cut adhesion testing.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDermott Wuchuan
Product: Pressure vessels and WHRU components including Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU stack, outlet duct, inlet duct, by-pass, and external seal-air duct
Position: NACE CIP Coating inspector
Reviewed documents and paint and coating materials.
Inspected surface preparation, environmental conditions, abrasive and compressed air, blasting, cleanliness, roughness, dust, soluble salts, paint mixing and thinning, wet-film thickness, and curing.
Performed visual and DFT inspection for each layer, paint-repair inspection, and pull-off and cross-cut adhesion testing.

Client: Jiangnan Boiler & Pressure Vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler & Pressure Vessel
Product: Waste Heat Boiler
Position: NACE CIP coating inspector
Reviewed documents.
Performed post-blasting cleanliness and roughness inspection.
Performed curing inspection, visual and DFT inspection for each layer, paint-repair inspection, cross-cut adhesion inspection, and final and marking inspection.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Third-Party Inspection
Pressure Vessel Inspection
Welding Inspection
Coating / Painting Inspection
Mechanical Inspection
NDT Inspection
Steel Structure Inspection
Subsea Product Inspection
Package and Skid Inspection
Vendor Surveillance
Document Review
Quality Control Document Review
Construction Inspection
Inspection Coordination

COMMODITIES
Pressure Vessels
FPSO Topsides
Subsea Structures
Steel Structures
Pipes and Tubes
Piping
Pipe Fittings
Valves
Chains
Bridge Steel
Steel Plates
Forgings
Skids
Gas Turbine Cylinders
Cranes
Structural Steel
Dynamic Equipment
Containers
Bridges
Anodes
Mooring Equipment
Ropes
Heat Exchangers
Separators
Scrubbers
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