
ANDY DU

SUMMARY
Andy Du is an inspection professional with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has performed resident and mechanical inspection on major projects involving pressure vessels, process and FPSO skids, gas turbine cylinders, dynamic equipment, piping, valves, subsea products, bridges, cranes, and other industrial equipment. His scope includes raw material, welding, NDT, dimensional and visual inspection, pressure and leak testing, coating, FAT, MRB review, packing, preservation, and final inspection. Andy has worked with contractors, manufacturers, clients, and end users including TEN/Total, Veolia, Sinopec, CNOOC, SLB, Modec, Baker Hughes, KOC, SBM, and HHI. He is experienced with international standards and welding processes including SAW, SMAW, GTAW, FCAW, and GMAW.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed material, mechanical, welding, coating, subsea, pressure vessel, steel structure, crane, bridge, piping, valve, and third-party inspection across major industrial projects.
Inspected raw materials, fabrication, welding, NDT, dimensional and visual condition, pressure and leak testing, coating, FAT, MRB documentation, packing, preservation, and final condition.
Coordinated inspection activities between contractors, manufacturers, clients, end users, and suppliers.

PROJECTS

Client: TEN (End user Total)
GRANMORU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and nozzle welding to shells and heads.
Witnessed NDT, hydrostatic testing, and weighing tests.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, painting, and nameplates.
Reviewed MRB documentation and inspected marking, packing, and preservation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection of flanges, elbows, and forgings.
Monitored clad welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Performed visual inspection, clad thickness inspection, PMI testing, and witnessed NDT.
Reviewed project documentation.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection.
Inspected formed heads, fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, consumables, welding parameters, welder qualification, and protection.
Inspected openings, nozzle fit-up and welding to shells and heads.
Witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, painting, and nameplates.
Witnessed weighing tests, reviewed MRB documentation, and inspected marking and packing.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material and formed-head inspection.
Inspected fit-up and tack welding, marking and openings, and nozzle fit-up and welding to shells and heads.
Performed chemical analysis of cladding and witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, nameplates, weighing, marking, and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material, formed-head, fit-up, tack welding, and welding process inspection.
Inspected marking, openings, nozzle fit-up and welding to shells and heads.
Performed PWHT inspection and witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, painting, and nameplates.
Witnessed weighing tests, reviewed MRB documentation, and inspected marking and packing.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material, formed-head, fit-up, tack welding, and material traceability inspection.
Monitored welding in accordance with WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected openings, nozzle fit-up and welding, PWHT, NDT, internal cleaning, and visual and dimensional condition.
Witnessed air-tight leak and hydrostatic tests.
Inspected pickling and passivation, blasting and painting, nameplates, final condition, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material, formed-head, material cutting, and traceability inspection.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding to WPS and PQR requirements.
Inspected nozzle fit-up and welding, PWHT, NDT, internal cleaning, and visual and dimensional condition.
Witnessed PMI, hardness, air-tight leak, hydrostatic, and weighing tests.
Inspected pickling and passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material, formed-head, material cutting, and traceability inspection.
Inspected fit-up and tack welding and monitored GTAW, FCAW, SMAW, SAW, and overlay welding to WPS and PQR requirements.
Inspected nozzle fit-up and welding, PWHT, NDT, internal cleaning, and visual and dimensional condition.
Witnessed PMI, hardness, air-tight leak, hydrostatic, and weighing tests.
Inspected pickling and passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material, formed-head, fit-up, tack welding, and welding process inspection.
Inspected marking, openings, nozzle fit-up and welding, and post-weld visual and dimensional condition.
Performed heat treatment inspection and witnessed hydrostatic testing.
Inspected blasting and painting, final condition, package shipping, and preservation.
Reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic testing and performed cleanliness inspection.
Performed final inspection and inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material, dimensional, and visual inspection.
Witnessed hydrostatic and helium/nitrogen leakage testing.
Performed final inspection and inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspector
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication and installation of structures, piping spools, valves, and other free-issue items.
Performed dimensional and visual inspection, hydrostatic testing, flange management, and mechanical completion checks.
Inspected blasting and painting and witnessed FAT testing.
Performed final inspection and inspected package shipping and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspector
Monitored feed gas heater and membrane housing fabrication.
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Witnessed NDE and hydrostatic testing and performed dimensional and visual inspection.
Inspected blasting and painting, insulation, flange management, and mechanical completion.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Witnessed FAT testing and performed final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspector
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system leak, FAT, and weighting and COG tests.
Performed dimensional and visual inspection and inspected blasting, painting, insulation, and flange management.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Performed mechanical completion and final inspection and inspected package shipping and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspector
Performed raw material and vessel fabrication inspection.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system leak, FAT, and weighting and COG tests.
Performed dimensional inspection and inspected blasting, painting, insulation, and flange management.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Performed mechanical completion and final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspector
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Witnessed NDE, hydrostatic, system leak, FAT, and weighting and COG tests.
Performed dimensional inspection and inspected blasting, painting, insulation, and flange management.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Performed mechanical completion, final inspection, package shipping, and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspector
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Witnessed NDE, hydrostatic, system leak, FAT, and weighting and COG tests.
Performed dimensional inspection and inspected blasting, painting, insulation, and flange management.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Performed mechanical completion and final inspection and inspected package shipping and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspector
Performed raw material inspection covering structure, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Witnessed NDE, hydrostatic, system leak, FAT, and weighting and COG tests.
Performed dimensional inspection and inspected blasting, painting, insulation, and flange management.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Performed mechanical completion and final inspection and inspected package shipping and preservation.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspector
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Performed parts machining quality, fit-up, and welding inspection.
Witnessed function, vibration, and noise tests.
Reviewed documentation and inspected package shipping and preservation.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface cleanliness before blasting, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, soluble salts, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface cleanliness before blasting, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, soluble salts, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed coating documentation and coating system qualification.
Inspected paint and coating materials, surface cleanliness, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, soluble salts, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed coating documentation.
Performed visual examination and DFT inspection.
Inspected paint repairs and adhesion using pull-off and crosscut tests.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documentation and inspected pickling and passivation.
Reviewed coating system qualification and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface condition before blasting, environmental conditions, abrasive and compressed air, and blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and adhesion inspection using pull-off and crosscut tests.

Client: Jiangnan Boiler & Pressure Vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler & Pressure Vessel
Position: NACE CIP coating inspector
Reviewed documentation and inspected cleanliness after blasting, including cleanliness degree, roughness, and dust.
Performed curing inspection and visual and DFT inspection for each layer.
Inspected paint repairs, crosscut adhesion, and final marking.

Client: Baker Hughes
Subsea product inspection
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: XT system products; Connections system products; GFDS System products
Position: Inspector
Inspected XT system tree frames, protection structures, debris caps, debris canopies, and shipping skids.
Inspected Connections system clamp connectors, pressure caps, vent caps, and light-duty clamps.
Inspected GFDS system porch, termination, male hub, and pup-piece products.
Performed raw material, MTR, receipt, cutting, marking, machining, fit-up, welding, UT, MT, visual, dimensional, coating, painting, adhesion, holiday, assembly, FAT, final, MRB, packing, and shipping inspection.
Inspected clad welding, PMI, CRA thickness, NDT, hardness, load testing, hydrostatic testing, gas testing, electrical continuity, back-seal testing, weight, and COG.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Third party inspection and certification of Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS and welded pipes, 5D inducted bends, stainless steel SMLS and welded tubes, nickel alloy pipes, square and rectangular tube, Cu alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Position: Third party inspector
Performed manufacturing procedure qualification test inspection.
Inspected chemical analysis and mechanical property testing.
Witnessed hydrostatic and NDT testing, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection and inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Third party inspection of Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM blind flange, flange, reducer, tee, elbow, weldolet, coupling, thread end cap, sockolet, nipple, etc.
Standards: ASME B16.5, ASME B16.9, ASME B16.11, MSS SP-97
Position: Third party inspector
Reviewed documentation and inspected chemical analysis and mechanical property testing.
Performed hardness and PMI testing.
Performed dimensional and visual quality inspection and inspected packing, marking, and coating.

Client: Neway Valve Plant, O&G Engineering, KOGAS, Rotary Engineering
Third party inspection of Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Position: Third party inspector
Reviewed documentation and performed PMI and mechanical property testing.
Performed hardness testing and witnessed PT, MT, UT, and RT.
Performed assembly, visual, and dimensional inspection.
Witnessed hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
Third party inspection of SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Product: SubSurface Safety Valve and Packer
Standards: API 14A, API 11D
Position: Third party inspector
Reviewed documentation and witnessed drift and function tests.
Performed dimensional and visual inspection.
Inspected marking, coating, and protection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Third party inspection of Steel plates and forging
Product: Shipped steel plates, spheroidal graphite cast iron, AISI 4130 and 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Position: Third party inspector
Reviewed documentation and inspected chemical analysis and mechanical property testing.
Performed hardness testing and witnessed UT and MT.
Performed visual and dimensional inspection and inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Third party inspection of Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspector
Reviewed documentation and inspected chemical analysis and mechanical property testing.
Witnessed proof load and break load testing.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Third party inspection of Anodes
Product: Al Anode, Zn Anode
Position: Third party inspector
Reviewed documentation and monitored casing.
Performed chemical and electrochemical analysis.
Performed crosscut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai Sailfish Rope, Shandong Rope Technology
Third party inspection of Other products
Product: Electric heater core, life raft, pick-up buoys, anchor buoys, polyamide (Nylone) 8-strand ropes
Position: Third party inspector
Reviewed documentation and witnessed hydrostatic, performance, and break load tests.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC (Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Containers
Position: Inspector
Reviewed documentation and inspected floorboards and corner fittings by sampling.
Witnessed relevant tests and performed routing inspection of welding, assembly, and dimensions.
Performed visual quality inspection after welding and coating inspection.
Witnessed general prototype testing and performed whole-container inspection.

Client: NP QHG Port, PSA Corporation Ltd, MEPT, Voltritermianal Europa S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA Panama International, Terminal S.A. (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container cranes (RTG/STS), offshore crane, hydraulic slewing crane
Position: Inspector
Reviewed quality documents and procedures, including WPS, welder qualifications, and drawings.
Performed raw material re-inspection.
Inspected main structure assembly, pre-welding, welding processes, and final structure condition.
Performed visual quality and coating inspection.
Witnessed FAT and EFAT of cranes.

Experience in the construction of bridges
Product: Steel bridges (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Position: CWI inspector
Performed raw material re-inspection.
Inspected mechanical properties and product chemical analysis for steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding, welding processes, visual quality after welding, and zinc coating of fabricated products.

Client: Samsung Engineering Co., Ltd, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland condenser and handing clamp
Position: Inspector
Reviewed quality control documents, including ITP, WPS/PQR, WQT, and NDT records.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing and cleaning and dry checks.
Witnessed surface preparation and performed visual and dry film checks.
Inspected rust prevention, including VCI application inside the gland condenser.
Performed visual and dimensional inspection, including nameplates.
Inspected packing and marking and reviewed manufacturing final inspection certificates.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Third-Party Inspection
Mechanical Inspection
Welding Inspection
Coating Inspection
NDT Inspection
Pressure Vessel Inspection
Steel Structure Inspection
Subsea Product Inspection
Piping and Valve Inspection
QA/QC Document Review
Vendor Surveillance
FAT and EFAT Inspection
Expediting and Client Coordination

COMMODITIES
Pressure Vessels
FPSO Topsides
Subsea Structures
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridge Steel
Steel Plates
Forgings
Gas Turbine Cylinders
Process Skids
Pumps
Membrane Skids
TEG Vessels
TEG Exchangers
Cranes
Containers
Anodes
Ropes
Safety Valves
Packers
Dynamic Equipment
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