
ANDY DU

SUMMARY
Andy Du has 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structure monitoring, crane monitoring, pressure vessel inspection, and third-party inspection. He has worked on major projects involving pressure vessels, gas turbine cylinders, packages and skids, dynamic equipment, subsea products, piping, valves, steel products, chains, cranes, containers, bridges, and equipment. His standards knowledge includes BSEN, ASME, ASTM, API, AWS D1.1, AWS D1.5, NORSOK, NACE, Classification Society Rules, and other international and national standards. Andy has extensive experience with SAW, SMAW, GTAW, FCAW, and GMAW welding processes, as well as coating inspection, NDT, hydrostatic testing, FAT, document review, and MRB review. He is experienced in coordinating effectively between contractors and clients on major projects.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed material, mechanical, welding, coating, pressure vessel, subsea product, package, skid, crane, bridge, container, and third-party inspection across major industrial projects.
Inspected raw materials, fabrication, welding, NDT, dimensional and visual condition, pressure and performance testing, coating, assembly, FAT, packing, marking, and preservation.
Reviewed ITPs, WPS/PQR, WQT, NDT records, MTRs, certificates, MRBs, and other quality documentation.
Coordinated inspection activities between contractors, manufacturers, clients, suppliers, and end users.

PROJECTS

Client: TEN (End user Total)
GRANMORU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, fit-up, tack welding, gaps, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and nozzle welding to shells and heads.
Witnessed NDT, hydrostatic testing, and weighing tests.
Inspected internal cleaning, visual and dimensions, pickling and passivation, painting, and nameplates.
Reviewed MRB documentation and inspected marking, packing, and preservation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection of flanges, elbows, and forgings.
Monitored clad welding, including preheat, consumables, welding parameters, welder qualification, and protection.
Performed visual inspection, clad thickness inspection, PMI testing, and witnessed NDT.
Performed document review.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and receipt inspection.
Inspected formed heads, fit-up, tack welding, gaps, alignment, and cleanliness.
Monitored welding processes, including preheat, consumables, welding parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and welding to shells and heads.
Witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional conditions, pickling and passivation, painting, and nameplates.
Witnessed weighing tests and reviewed MRB documentation.
Inspected final marking and packing.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Performed chemical analysis of cladding and witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional conditions, pickling and passivation, and nameplates.
Witnessed weighing tests, reviewed MRB documentation, and inspected marking and packing.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Monitored welding processes and performed PWHT inspection.
Witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional conditions, pickling and passivation, and nameplates.
Witnessed weighing tests, reviewed MRB documentation, and inspected marking and packing.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Monitored welding to WPS and PQR requirements using GTAW, FCAW, SMAW, SAW, and overlay welding.
Performed PWHT inspection and witnessed NDT, air-tight leak tests, and hydrostatic tests.
Inspected internal cleaning, visual and dimensional conditions, pickling and passivation, blasting and painting, and nameplates.
Performed final inspection, weighing, MRB review, and marking and packing inspection.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material inspection, material cutting, traceability, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Monitored welding to WPS and PQR requirements using GTAW, FCAW, SMAW, SAW, and overlay welding.
Witnessed PMI, hardness, NDT, air-tight leak, hydrostatic, and weighing tests.
Performed PWHT, internal cleaning, visual and dimensional, pickling and passivation, and nameplate inspection.
Reviewed MRB documentation and inspected marking and packing.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material inspection, material cutting, traceability, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Monitored GTAW, FCAW, SMAW, SAW, and overlay welding to WPS and PQR requirements.
Witnessed PMI, hardness, NDT, air-tight leak, hydrostatic, and weighing tests.
Performed PWHT, internal cleaning, visual and dimensional, pickling and passivation, and nameplate inspection.
Reviewed MRB documentation and inspected marking and packing.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material, formed head, fit-up, tack welding, marking, opening, and nozzle inspection.
Monitored welding processes and performed post-weld visual, dimensional, and heat treatment inspection.
Witnessed hydrostatic testing and performed blasting and painting inspection.
Performed final inspection, package shipping and preservation inspection, and MRB review.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material, dimensional, visual, cleanliness, and final inspection.
Witnessed hydrostatic testing and inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material, dimensional, visual, and final inspection.
Witnessed hydrostatic and helium/nitrogen leakage tests.
Inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspector
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Performed dimensional and visual inspection, hydrostatic testing, blasting and painting inspection, and flange management inspection.
Monitored structure, piping spool, valve, and free-issue installation.
Performed mechanical completion checks, FAT, final inspection, and package shipping and preservation inspection.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspector
Monitored feed gas heater and membrane housing fabrication.
Inspected raw materials, structures, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Performed NDE, dimensional and visual inspection, hydrostatic testing, blasting and painting inspection, and flange management.
Monitored installation and performed mechanical completion, insulation, FAT, and final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspector
Inspected raw materials including structures, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Performed NDE, dimensional and visual inspection, hydrostatic testing, blasting and painting inspection, and flange management.
Monitored installation and performed mechanical completion, insulation, FAT, system leak, weighting and COG, final inspection, and package shipping and preservation inspection.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspector
Inspected raw materials and vessel fabrication.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Performed NDE, dimensional, hydrostatic, blasting and painting, and flange management inspection.
Monitored installation and performed mechanical completion, insulation, FAT, system leak, weighting and COG, and final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspector
Inspected raw materials including structure, piping, valves, and piping fittings.
Monitored structure and piping spool fabrication, including monorails and lifting lugs.
Performed NDE, dimensional, hydrostatic, blasting and painting, and flange management inspection.
Monitored installation and performed mechanical completion, insulation, FAT, system leak, weighting and COG, final inspection, and package shipping and preservation inspection.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspector
Inspected raw materials and monitored structure and piping spool fabrication.
Performed NDE, dimensional, hydrostatic, blasting and painting, and flange management inspection.
Monitored installation and performed mechanical completion, insulation, FAT, system leak, weighting and COG, final inspection, and package shipping and preservation inspection.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspector
Inspected raw materials and monitored structure and piping spool fabrication.
Performed NDE, dimensional, hydrostatic, blasting and painting, and flange management inspection.
Monitored installation and performed mechanical completion, insulation, FAT, system leak, weighting and COG, and final inspection.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface cleanliness, abrasive and compressed air, environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, DFT, paint repairs, and adhesion by pull-off and crosscut testing.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed coating documentation and inspected paint and coating materials.
Inspected surface preparation, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents and coating system qualification.
Inspected coating materials, surface preparation, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed coating documentation.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents and coating system qualification.
Performed pickling and passivation inspection and inspected coating materials, surface preparation, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed coating documents and inspected coating materials, surface preparation, abrasive and compressed air, environmental conditions, blasting, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed documents and inspected coating materials, surface preparation, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, soluble salts, paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection, paint repair inspection, and pull-off and crosscut adhesion testing.

Client: Jiangnan Boiler &Pressure vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler &Pressure vessel
Position: NACE CIP coating inspector
Reviewed documents and inspected cleanliness after blasting, including cleanliness, roughness, and dust.
Performed curing, visual and DFT inspection for each layer, paint repair, crosscut adhesion, and final and marking inspection.

Client: Baker Hughes
Working Experience on Subsea product For Baker Hughes
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: XT system products; Connections system products; GFDS System products
Position: Subsea product inspector
Inspected raw materials, material cutting and marking, machining, fit-up, welding, weld UT and MT, weld visual condition, and base-frame dimensions.
Inspected coating preparation, painting, adhesion, holiday testing, assembly, FAT, final inspection, MRB, and package shipping.
Inspected clad welding, PMI, CRA thickness, NDT, hardness, dimensions, load tests, hydrostatic and gas tests, electrical continuity, back seal tests, weight, visual condition, COG, and final documentation.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Third party inspection & Certification of: Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Position: Third party inspector
Performed manufacturing procedure qualification testing and product chemical and mechanical property testing.
Witnessed hydrostatic and NDT testing including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection and inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Standards: ASME B16.5 ASME B16.9, ASME B16.11, MSS SP-97
Position: Third party inspector
Performed document review, chemical analysis, mechanical property testing, hardness testing, PMI testing, and dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Position: Third party inspector
Performed document review, PMI, mechanical property, hardness, and NDT testing including PT, MT, UT, and RT.
Performed assembly, visual and dimensional inspection, hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Standards: API 14A, API 11D
Position: Third party inspector
Reviewed documents and witnessed drift and function testing.
Performed dimensional, visual, marking, coating, and protection inspection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Position: Third party inspector
Performed document review, chemical analysis, mechanical property, and hardness testing.
Witnessed UT and MT and performed visual and dimensional inspection.
Inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspector
Performed document review, chemical analysis, and mechanical property testing.
Witnessed proof load and break load tests.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Position: Third party inspector
Reviewed documents and monitored casing.
Performed chemical and electrochemical analysis, cross-cut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Position: Third party inspector
Performed document review, hydrostatic and performance testing, and break load testing.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Containers
Position: Container inspector
Reviewed documents and inspected floorboards and corner fittings by sampling.
Witnessed relative testing, routing inspection, welding, assembly, and dimensional inspection.
Performed post-weld visual quality, coating, general prototype, and whole-container inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Position: Heavy lifting equipment inspector
Reviewed quality documents and procedures including WPS, welder qualifications, and drawings.
Performed raw material re-inspection and inspected main structure assembly, pre-welding, and welding processes.
Performed post-weld visual quality, structure final, and coating inspection.
Witnessed FAT and EFAT of cranes.

Experience in the construction of bridges
Product: Steel bridges (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Position: CWI inspector
Performed raw material re-inspection and mechanical property and product chemical analysis for steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding, welding processes, post-weld visual quality, and zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland Condenser & Handing Clamp
Position: Equipment inspector
Reviewed quality control documents including ITP, WPS/PQR, WQT, and NDT records.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing, cleaning and dry checks, and surface preparation.
Performed visual and dry film checks, rust prevention inspection, dimensional and nameplate inspection, and packing and marking inspection.
Reviewed manufacturing final inspection documentation.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Steel Structure Inspection
Pressure Vessel Inspection
FPSO Topside Inspection
Subsea Structure Inspection
Third-Party Inspection
Coating Inspection
Welding Inspection
NDT Inspection
Mechanical Inspection
Package and Skid Inspection
Vendor Inspection
Document Review
MRB Review
Crane Inspection
Bridge Inspection

COMMODITIES
Coating
Pressure Vessels
FPSO Packages
Subsea Products
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridges
Steel Plates
Forgings
Gas Turbine Cylinders
Packages and Skids
Pumps
Exchangers
Separators
Scrubbers
Cranes
Containers
Anodes
Ropes

fulkrum.com

image2.png
\




image200.png
\




