
ANDY DU

SUMMARY
Andy Du is an inspector with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has worked as a resident, mechanical, CWI, and NACE CIP coating inspector on major pressure vessel, FPSO, package, skid, subsea, bridge, crane, and dynamic-equipment projects. His experience covers international and national standards and welding processes including SAW, SMAW, GTAW, FCAW, and GMAW. He has extensive inspection and certification scope across pipes, fittings, valves, vessels, structures, chains, anodes, and other products, with strong coordination between contractors and clients on large projects.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed material, mechanical, welding, coating, pressure vessel, package, skid, subsea product, crane, bridge, container, and third-party inspection assignments.
Inspected equipment and products including pressure vessels, FPSO systems, subsea products, pipes and tubes, fittings, valves, steel plates and forgings, chains, anodes, cranes, and containers.
Coordinated inspection activities between contractors and clients on large projects.
Reviewed technical and quality documentation and witnessed testing, NDT, FAT, hydrostatic, load, leakage, and performance tests.

PROJECTS

Client: TEN (End user Total)
GRANMORU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Inspected raw materials, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shell and head.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic and weighing tests.
Inspected pickling and passivation treatment.
Inspected painting, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Inspected raw materials, including flanges, elbows, and forgings.
Monitored clad welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Performed visual and clad-thickness inspection.
Witnessed NDT and PMI tests.
Reviewed project documents.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Inspected raw materials, including MTR review and raw material receipt inspection.
Inspected formed heads, fit-up, tack welding, gaps, alignment, and cleanliness.
Monitored welding processes, including preheat, consumables, parameters, welder qualification, and protection.
Inspected marking, openings, nozzle fit-up, and nozzle welding to shell and head.
Witnessed NDT, hydrostatic, and weighing tests.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, painting, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Inspected raw materials, MTRs, and receipt condition.
Inspected formed heads, fit-up and tack welding, marking, openings, and nozzle fit-up and welding to shell and head.
Performed chemical analysis of cladding and witnessed NDT.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, nameplates, marking, and packing.
Witnessed hydrostatic and weighing tests.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Inspected raw materials, MTRs, and receipt condition.
Inspected formed heads, fit-up and tack welding, marking, openings, and nozzle fit-up and welding to shell and head.
Monitored welding and inspected PWHT.
Witnessed NDT and hydrostatic testing.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, painting, nameplate, marking, and packing.
Witnessed the weighing test and reviewed MRB documentation.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Inspected raw materials, MTRs, and receipt condition.
Inspected formed heads, material cutting and traceability, fit-up, and tack welding.
Monitored welding according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, nozzle fit-up and welding to shell and head, and PWHT.
Witnessed NDT, air-tight leak, and hydrostatic tests.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, blasting and painting, nameplates, final condition, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Inspected raw materials, MTRs, and receipt condition.
Inspected formed heads, material cutting and traceability, fit-up, and tack welding.
Monitored welding according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, nozzle fit-up and welding to shell and head, and PWHT.
Witnessed PMI, hardness, NDT, air-tight leak, hydrostatic, and weighing tests.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Inspected raw materials, MTRs, and receipt condition.
Inspected formed heads, material cutting and traceability, fit-up, and tack welding.
Monitored welding according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, nozzle fit-up and welding to shell and head, and PWHT.
Witnessed PMI, hardness, NDT, air-tight leak, hydrostatic, and weighing tests.
Inspected internal cleaning, visual and dimensional condition, pickling and passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Inspected raw materials and formed heads.
Inspected fit-up and tack welding, marking, openings, nozzle fit-up and welding to shell and head.
Monitored welding and performed post-weld visual inspection.
Performed dimensional and visual inspection and heat-treatment inspection.
Witnessed hydrostatic testing.
Inspected blasting, painting, final condition, package shipping, and preservation.
Reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Inspected raw materials.
Performed dimensional, visual, cleanliness, and final inspection.
Witnessed hydrostatic testing.
Inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Inspected raw materials.
Performed dimensional and visual inspection.
Witnessed hydrostatic and helium/nitrogen leakage tests.
Performed final inspection and inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspector
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, and lifting-lug fabrication.
Monitored piping spool fabrication and installation of structures, piping spools, valves, and other free-issue items.
Performed dimensional and visual inspection and flange-management inspection.
Witnessed hydrostatic and FAT tests.
Performed mechanical-completion and final inspection.
Inspected blasting, painting, package shipping, and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspector
Monitored feed-gas-heater and membrane-housing fabrication.
Inspected raw materials, structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic tests.
Performed dimensional and visual inspection, flange management, mechanical-completion inspection, insulation inspection, FAT, and final inspection.
Monitored installation of structures, piping spools, valves, and other free-issue items.
Inspected blasting, painting, and package shipping.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspector
Inspected raw materials, structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system-leak, and FAT tests.
Performed dimensional and visual inspection, flange management, mechanical-completion inspection, insulation inspection, and final inspection.
Inspected blasting, painting, package shipping, preservation, marking, and packing.
Performed weighing and COG inspection.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspector
Inspected raw materials, structure, piping, valves, and piping fittings.
Performed vessel fabrication inspection and monitored structure and piping spool fabrication.
Witnessed NDE, hydrostatic, system-leak, and FAT tests.
Performed dimensional inspection, flange management, mechanical-completion inspection, insulation inspection, final inspection, and weighing and COG inspection.
Inspected blasting and painting and monitored installation of structures, piping spools, valves, and other free-issue items.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspector
Inspected raw materials, structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system-leak, and FAT tests.
Performed dimensional inspection, flange management, mechanical-completion inspection, insulation inspection, final inspection, and weighing and COG inspection.
Inspected blasting, painting, package shipping, preservation, marking, and packing.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspector
Inspected raw materials, structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system-leak, and FAT tests.
Performed dimensional inspection, flange management, mechanical-completion inspection, insulation inspection, final inspection, and weighing and COG inspection.
Inspected blasting, painting, package shipping, and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspector
Inspected raw materials, structure, piping, valves, and piping fittings.
Monitored primary and secondary structure, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE, hydrostatic, system-leak, and FAT tests.
Performed dimensional inspection, flange management, mechanical-completion inspection, insulation inspection, final inspection, and weighing and COG inspection.
Inspected blasting, painting, package shipping, and preservation.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspector
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Inspected parts machining quality, fit-up and welding, and package shipping and preservation.
Witnessed function, vibration, and noise tests.
Reviewed documents.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed coating documents and inspected paint and coating materials.
Inspected surface cleanliness before blasting, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed coating documents and inspected paint and coating materials.
Inspected surface preparation, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents and coating-system qualification.
Inspected paint and coating materials, surface cleanliness, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed coating documents.
Performed visual and DFT inspection, paint-repair inspection, and adhesion inspection by pull-off and crosscut tests.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents and coating-system qualification.
Inspected pickling and passivation, paint and coating materials, surface preparation, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface preparation, abrasive and compressed air, environmental conditions, and blasting cleanliness.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface preparation, environmental conditions, abrasive and compressed air, and blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, curing, visual condition, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut tests.

Client: Jiangnan Boiler &Pressure vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler &Pressure vessel
Position: NACE CIP coating inspector
Reviewed documents.
Performed cleanliness checks after blasting, including cleanliness, roughness, and dust.
Inspected curing, visual condition and DFT for each layer, paint repairs, and crosscut adhesion.
Performed final and marking inspection.

Client: Baker Hughes
Subsea product
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: XT system products, Connections system products, and GFDS System products
Inspected raw materials, MTRs, and receipt condition.
Inspected material cutting, marking, machining, fit-up, welding, dimensions, and assembly.
Witnessed UT and MT of welds and inspected clad welding, PMI, CRA thickness, NDT, and hardness.
Inspected coating surface preparation, painting, adhesion, and holiday testing.
Witnessed load, hydrostatic, gas, and FAT tests, including weight, visual, electrical continuity, back-seal, and COG tests.
Performed final, MRB, package, and shipping inspection.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Performed manufacturing procedure qualification testing.
Inspected product chemical analysis and mechanical-property testing.
Witnessed hydrostatic and NDT tests, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Reviewed documents.
Inspected product chemical analysis and mechanical-property testing.
Performed hardness, PMI, dimensional, and visual quality inspection.
Inspected packing, marking, and coating.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Reviewed documents.
Witnessed PMI, mechanical-property, hardness, and NDT tests, including PT, MT, UT, and RT.
Performed assembly, visual, and dimensional inspection.
Witnessed hydraulic, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Product: SubSurface Safety Valve & Packer
Reviewed documents.
Witnessed drift and function inspections.
Performed dimensional, visual, marking, coating, and protection inspection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Reviewed documents.
Inspected chemical analysis, mechanical-property testing, and hardness.
Witnessed UT and MT.
Performed visual and dimensional inspection.
Inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Reviewed documents.
Inspected chemical analysis and mechanical-property testing.
Witnessed proof-load and break-load tests.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Reviewed documents.
Monitored casing.
Inspected chemical and electrochemical analysis, cross-cut, resistance, weight, dimensional, and visual quality.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Reviewed documents.
Witnessed hydrostatic, performance, and break-load tests.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Container
Reviewed documents.
Inspected floorboard and corner-fitting samples.
Witnessed relative tests and general prototype testing.
Performed routing inspection of welding, assembly, and dimensions.
Performed visual quality, coating, whole-container, and final inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Reviewed related documents and procedures, including WPS, welder qualification, and drawings.
Performed raw-material re-inspection.
Inspected main structure steel assembly, pre-welding, welding processes, and final structure condition.
Performed visual quality and coating inspection.
Witnessed FAT and EFAT of cranes.

Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Product: Steel bridge
Position: CWI inspector
Performed raw-material re-inspection.
Inspected mechanical properties and chemical analysis of steel plates, bolts, and nuts.
Witnessed welding-procedure qualification and welder-qualification tests.
Inspected pre-welding and welding processes and visual quality after welding.
Checked zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Construction of Equipment
Product: Gland Condenser & Handing Clamp
Reviewed quality-control documents, including ITP, WPS/PQR, WQT, and NDT.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing and cleaning and dry checks.
Witnessed surface preparation and performed visual and dry-film checks.
Inspected rust prevention, including VCI application inside the gland condenser.
Performed visual and dimensional inspection, including nameplates.
Inspected packing and marking and reviewed the manufacturing final inspection.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Steel Structure Inspection
Pressure Vessel Inspection
FPSO Topside Inspection
Subsea Structures Monitoring
Crane Inspection
Third-Party Inspection and Certification
Welding Inspection
Coating Inspection
Mechanical Inspection
Package and Skid Inspection
NDT Coordination
Document Review
Contractor and Client Coordination

COMMODITIES
Coating
Pressure Vessels
FPSO Topside
Subsea Products
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridge Steel
Plates and Forgings
Gas Turbine Cylinders
Packages and Skids
Pumps
Membrane Housings
Heat Exchangers
Separators
Scrubbers
Cranes
Containers
Anodes
Wire Rope Slings
Ropes
Gland Condensers
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