
ANDY DU

SUMMARY
Andy Du is an inspection professional with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structure monitoring, crane monitoring, pressure vessels, and third-party inspection. He has performed resident and mechanical inspection on pressure vessels, gas turbine cylinders, packages, skids, dynamic equipment, and major FPSO-related projects. His background includes coating inspection covering surface preparation, blasting, paint application, curing, dry film thickness, repair, and adhesion assessment, together with inspection of subsea XT, connections, and GFDS products. Andy has broad knowledge of international and national standards and guidelines, including ASME, ASTM, API, AWS, NACE, and classification society rules, and is experienced in SAW, SMAW, GTAW, FCAW, and GMAW welding processes. He is also experienced in coordinating contractors and clients on major projects.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO

WORK EXPERIENCE

PROJECTS

	LOCATION
	Zhenjiang, Jiangsu Province, China

	EDUCATION
	2005~2008 University: Nanjing University of Technology

	LANGUAGES
	English (speaking, reading, writing, listening) Chinese (Native language)

	COMMODITIES/SPECIALTIES
	Coating Pressure vessel, Package FPSO Subsea product Steel structure Pipes &Tubes Piping Fittings, Valves, Chains Bridge Steel plates and forgings …

	CERTIFICATIONS/TRAINING
	2008: Training for CWI 2012: Training for Nace Coating Level II 2022: Training for UT/MT

	CODES/STANDARDS
	AWS, ASME, ASTM, API, GB, HB, JB, EN, ISO…



GRANMORU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Performed painting inspection.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd..
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection of flanges, elbows, and forgings.
Monitored the clad welding process, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Performed visual inspection.
Performed clad thickness inspection.
Witnessed NDT.
Witnessed PMI testing.
Reviewed documents.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Performed painting inspection.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed chemical analysis of cladding.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Monitored the welding process.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Monitored welding processes according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak and hydrostatic tests.
Inspected pickling and passivation treatment.
Performed blasting and painting inspection.
Verified nameplates.
Performed final inspection.
Inspected marking and packing.
Reviewed MRBs.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, material cutting, and traceability.
Inspected fit-up and tack welding.
Monitored welding processes according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness tests.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak and hydrostatic tests.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads, material cutting, and traceability.
Inspected fit-up and tack welding.
Monitored welding processes according to WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness tests.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak and hydrostatic tests.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRBs.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material inspection and formed-head inspection.
Inspected fit-up and tack welding.
Monitored welding processes.
Performed visual inspection after welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed dimensional and visual inspection.
Performed heat treatment inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Performed final inspection.
Inspected package shipping and preservation.
Reviewed MRBs.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material inspection.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed cleanliness inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material inspection.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Witnessed helium and nitrogen leakage testing.
Performed final inspection.
Inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management inspection.
Performed mechanical completion checks.
Witnessed FAT testing.
Performed final inspection.
Inspected package shipping and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspector
Monitored feed gas heater and membrane housing fabrication processes.
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Performed insulation inspection.
Witnessed FAT testing.
Performed final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Performed insulation inspection.
Witnessed FAT testing.
Witnessed system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Performed vessel fabrication inspection.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Performed insulation inspection.
Witnessed FAT testing.
Witnessed system leak testing.
Performed weighing and COG inspection.
Performed final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Performed insulation inspection.
Witnessed FAT and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional inspection.
Witnessed hydrostatic and system leak testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Performed insulation inspection.
Witnessed FAT testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspector
Performed raw material inspection of structure, piping, valves, and pipe fittings.
Monitored primary and secondary structure, monorails, and lifting lugs fabrication.
Monitored piping spool fabrication.
Witnessed NDE.
Performed dimensional inspection.
Witnessed hydrostatic and system leak testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Performed insulation inspection.
Witnessed FAT testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspector
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Performed parts machining quality inspection.
Inspected fit-up and welding.
Witnessed function, vibration, and noise tests.
Inspected package shipping and preservation.
Reviewed documents.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Inspected surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface cleanliness before blasting, abrasive, and compressed air.
Inspected environmental conditions, blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing, thinning, wet film thickness, curing, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents and coating system qualification.
Inspected paint and coating materials.
Inspected surface cleanliness, abrasive, compressed air, and environmental conditions before and during blasting.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing, thinning, wet film thickness, curing, visual examination, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed documents.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Inspected adhesion by pull-off and crosscut testing.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected pickling and passivation and coating system qualification.
Inspected paint and coating materials.
Inspected surface cleanliness, abrasive, compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing, thinning, wet film thickness, curing, visual examination, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents and paint and coating materials.
Inspected surface cleanliness, abrasive, compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing, thinning, wet film thickness, curing, visual examination, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Inspected surface cleanliness before blasting and environmental conditions.
Inspected abrasive and compressed air.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing, thinning, wet film thickness, curing, visual examination, and DFT.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: Jiangnan Boiler &Pressure vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler &Pressure vessel
Position: NACE CIP coating inspector
Reviewed documents.
Checked cleanliness after blasting, including cleanliness degree, roughness, and dust.
Performed curing inspection.
Performed visual examination and DFT inspection for each layer.
Inspected paint repairs.
Performed adhesion inspection by crosscut testing.
Performed final and marking inspection.

Subsea product For Baker Hughes - XT system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Tree frame, Protection structure, Debris cap, Debris Canopy, Shipping Skid
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected material cutting and marking.
Performed machining inspection.
Witnessed fit-up and monitored structural welding.
Witnessed UT and MT of welds.
Performed visual inspection of welds.
Verified base frame dimensions.
Inspected coating surface preparation, painting, adhesion, and holiday testing.
Performed assembly, FAT, and final inspection.
Reviewed MRBs.
Performed package and shipping inspection.

Subsea product For Baker Hughes - Connections system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Clamp connectors (VCCS &HCCS Type T, HCCS-L, Test Clamp), Pressure Caps, Vent caps, Light Duty Clamps
Performed raw material and machining inspection.
Performed NDT inspection before clad welding.
Monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT inspection.
Witnessed hardness testing.
Performed dimensional inspection.
Witnessed load testing.
Performed blasting and painting inspection.
Witnessed adhesion and holiday testing.
Performed assembly and FAT inspection, including weight, visual, electrical continuity, and COG tests.
Performed final inspection and reviewed MRBs.
Performed package and shipping inspection.

Subsea product For Baker Hughes - GFDS System
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Porch, Termination, Male Hub/pup-piece
Performed raw material and machining inspection.
Performed NDT inspection before clad welding.
Monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT inspection.
Performed dimensional inspection.
Witnessed hydrostatic and gas testing.
Performed blasting and painting inspection.
Witnessed assembly and FAT testing, including weight, visual, electrical continuity, and back seal tests.
Performed final inspection and reviewed MRBs.
Performed package and shipping inspection.

Pipe & tube
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Position: Third party inspection & Certification
Performed manufacturing procedure qualification testing.
Witnessed product chemical analysis and mechanical property testing.
Witnessed hydrostatic and NDT testing, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Pipe fittings
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed hardness and PMI testing.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Position: Third party inspection & Certification
Reviewed documents.
Witnessed PMI, mechanical property, hardness, and NDT testing, including PT, MT, UT, and RT.
Performed assembly, visual, and dimensional inspection.
Witnessed hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Position: Third party inspection & Certification
Reviewed documents.
Witnessed drift and function testing.
Performed dimensional, visual, marking, coating, and protection inspection.

Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis, mechanical property, hardness, UT, and MT testing.
Performed visual and dimensional inspection.
Performed painting, marking, and packing inspection.

Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed proof load and break load testing.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Position: Third party inspection & Certification
Reviewed documents.
Monitored casing.
Witnessed chemical and electrochemical analysis.
Performed crosscut, resistance, weight, dimensional, and visual quality inspection.

Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Position: Third party inspection & Certification
Reviewed documents.
Witnessed hydrostatic, performance, and break load testing.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Reviewed documents.
Performed floorboard and corner fitting sampling.
Witnessed relative testing.
Performed routing inspection of welding, assembly, and dimensions.
Performed visual quality inspection after welding.
Performed coating inspection.
Witnessed general prototype testing.
Performed whole-container inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Reviewed related documents and procedures, including WPS, welder qualification, and drawings.
Performed raw material re-inspection.
Inspected main structure steel assembly.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Performed structure final inspection and coating inspection.
Witnessed FAT and EFAT of cranes.

Experience in the construction of bridges
Product: Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Position: CWI inspector
Performed raw material re-inspection.
Witnessed mechanical property testing and product chemical analysis of steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Checked zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland Condenser & Handing Clamp
Reviewed quality control documents, including ITP, WPS/PQR, WQT, and NDT.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing.
Witnessed cleaning and dry checks.
Witnessed surface preparation.
Performed visual and dry film checks.
Inspected rust prevention, including VCI application inside the gland condenser.
Performed visual and dimensional inspection, including nameplates.
Inspected packing and marking.
Reviewed manufacturing final inspection.
| NACE CIP Level II |
| CWI Certificate |
| ASNT UT level 2 certificate |
| ASNT MT level 2 certificate |

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Steel Structure Inspection
Pressure Vessel Inspection
FPSO Topside Inspection
Subsea Structure Monitoring
Crane Inspection
Third-Party Inspection
Coating / Painting Inspection
Welding Inspection
Mechanical Inspection
Package and Skid Inspection
NDT Coordination
Document Review
Fabrication Monitoring
Quality Control Document Review
Contractor and Client Coordination

COMMODITIES
Pressure Vessels
FPSO Topside Structures
Subsea Products
Steel Structures
Pipes and Tubes
Piping
Pipe Fittings
Valves
Chains
Bridges
Steel Plates
Forgings
Gas Turbine Cylinders
Packages
Skids
Pumps
Membrane Housings
Separators
Scrubbers
Exchangers
Cranes
Wire Rope Slings
Anodes
Containers
Gland Condensers
Handing Clamps
Subsea Safety Valves
Packers
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