
VIMLESH KUMAR MISHRA

SUMMARY
Vimlesh Kumar Mishra is an Inspection Engineer with more than 21 years of experience across pipe plants, coating plants, coil and plate mills, pressure vessels, piping, equipment erection and expediting. He has more than 12 years of QA/QC experience in pipe manufacturing organizations and more than 9 years of third-party inspection experience covering oil and gas, petrochemical and construction projects. His expertise includes steel pipe, welding, coating and NDE inspection, as well as static and pressure-containing equipment such as pressure vessels, heat exchangers, storage tanks, columns and reactors. He prepares and reviews quality plans, WPS, PQR and WPQR documentation, monitors fabrication and NDE activities, interprets radiographs and provides technical recommendations for inspection findings and remediation.

EDUCATION
Diploma in Mechanical Engineering

QUALIFICATIONS AND TRAINING
ASNT Level-II in Eddy Current Testing (ECT)
Welding Inspector Technology (WT)
ASNT UT Level II
ASNT VT Level II
ASNT MT Level II
ASNT RT Level II
ASNT PT Level II

PREVIOUS WORK HISTORY WITH FULKRUM
SS pipes and tube inspection for M/s Oil SERV, with Venus Pipes and Tubes Limited as manufacturer; scope included RMTC, raw material, heat-treatment, mechanical and chemical test review, hydrostatic testing and pipe dimensional inspection.

CODES AND STANDARDS
ASME Section IX
AWS
B31.3
B31.1
B31.2
B31.4
B31.8
API 1104
API 650
API 510
API 570
ISO 15590-1
MSS-SP-75
ASME B16.49
API 5L
ASME Section V-2015
ISO 10893-9-2011
EN BS 5996
EN 10246-15
ASTM A435
ASTM A578
SEL072
ISO 10893-11-2011
ASTM E273
ASTM E164-2013
ASTM E587-10
ISO 10893-8-2011
ASTM E213-2014
ASTM E94-2010
ISO 19232-2013
ASTM E1815-08
ISO 11699-2008
ASTM SE-1079-2010
ISO 10893-6:2011
ISO 10893-5-2011
ASTM E-709:2014
ASME Section VIII Division I and Division II
ASME Section II
API 571
API 574
API 576
API 577
API 578
API 653
ASME PCC-2
ASME B31.1 & B31.3
API 5L & API 1104
AWS D1.1 & IS 7215
ASME B16.5
ISO 21809-5
ISO/IEC 17025
PED 2014/68/EU
EN 287-1
ISO 9606-1
EN 15614
CFR49 (DOT4L)
IS 3589
ASTM A370
ASTM A751
DIN
BGS
SHELL

WORK EXPERIENCE

MAR 2018 – OCT 2018
LOYAL EQUIPMENTS LIMITED
QUALITY SR. ENGINEER
Reviewed and verified material test certificates, material identification and heat-number transfer against codes, standards, specifications and drawings.
Monitored manufacturing activities for compliance with drawings, codes, allowable tolerances and approved quality control plans.
Performed visual and dimensional fit-up inspection, including root gap, root face, bevel angle, joint cleanliness and preheating requirements.
Surveilled welding parameters, interpass temperature, electrode handling, backing and filler-wire control in accordance with WPS requirements.
Inspected SMAW, GTAW, FCAW and SAW welds for undercut, reinforcement, surface porosity, underfill and lack of fusion.
Witnessed PMI, hardness testing, thickness measurement, PWHT and reviewed PWHT charts.
Witnessed final dimensional and visual inspection and prepared inspection reports for client approval.
Verified UT, RT, MPT and LPT results before hydro testing.
Witnessed hydrostatic, pneumatic and vacuum testing in accordance with approved procedures and specifications.
Performed stage-wise fit-up, dimensional, visual, assembly and alignment inspection.
Performed final inspection after hydro testing, including internal cleaning, flange-face cleaning and nameplate fixing.
Reviewed final MRB/manufacturing data books and dossiers and submitted them to the client/TPI for approval.
Inspected incoming plates, pipes, fittings, flanges, valves and compressor parts.
Reviewed as-built drawings and obtained AI/TPI signatures.
Coordinated with third-party inspectors including TUV, Lloyd’s, BVIS, SGS and Intertek.
Communicated corrective actions for non-conformance reports and ensured fulfilment of inspection and test requirements at all stages.
Inspected piping spools and consoles against P&I diagrams and maintained inspection records and final ISO/U-Stamp documentation.
Reviewed vendor quality plans for forgings, pipes, fittings, tubes, tube sheets, baffles and tube bundles.
Performed external vendor inspection for tube sheets, baffles, tubes and tube bundles.
Coordinated TPI and test-agency calls and laboratory instrument calibration.

AUG 2017 – MAR 2018
SUPERTECH INFRAPROJECTS PVT, LTD
QUALITY ENGINEER
Performed pre-assembly and alignment activities for boiler structures, pressure parts and piping.
Reviewed isometric and GA drawings and inspected material identification against applicable codes and specifications.
Inspected fit-up and welding and prepared fit-up and weld visual reports.
Inspected NDT activities and reviewed NDT reports and heat-treatment reports.
Prepared punch lists and line history sheets.
Witnessed hydro testing of boiler pressure parts and piping systems.
Operated PMI machine and D. Meter for material identification and thickness inspection.
Prepared welding schedules for pressure-part and piping joints in accordance with IBR and ASME codes.
Attended weekly and monthly meetings with the client and ensured work was performed safely and according to quality and health and safety procedures.

SEP 2007 – JUL 2017
WELSPUN CORP LIMITED
QA/QC
Prepared and implemented QA/QC procedures and Quality Assurance & Inspection Test Plans according to client technical specifications, including API, ASTM, DIN, BGS, ISO and SHELL requirements.
Monitored shift-wise, stage-wise, size-wise and line-wise production and consumption reports.
Documented and implemented ISO 9001:2000 requirements and certification activities in accordance with the Quality System Manual and Quality System Procedures.
Liaised with TPI, clients and consultants on quality systems, procedures and project coordination.
Applied required specifications and coordinated inspection and testing equipment, materials and manpower for projects.
Handled customer complaints relating to quality matters.

OCT 2005 – AUG 2007
MAN INDUSTRIES INDIA LIMITED
QA/QC
Prepared and implemented QA/QC procedures and Quality Assurance & Inspection Test Plans according to client technical specifications, including API, ASTM, DIN, BGS, ISO and SHELL requirements.
Monitored shift-wise, stage-wise, size-wise and line-wise production and consumption reports.
Documented and implemented ISO 9001:2000 requirements and certification activities in accordance with the Quality System Manual and Quality System Procedures.
Liaised with TPI, clients and consultants on quality systems, procedures and project coordination.
Applied required specifications and coordinated inspection and testing equipment, materials and manpower for projects.
Handled customer complaints relating to quality matters.

PROJECTS

	Name of Employer
	Name of Client
	Name of Project
	Name of Manufacturer
	Size & Specification of Pipe (Including Grade, HSAW/ LSAW/HFERW) OR DFBE and 3LPE Coating
	Man Inspection activities.& Qty/ (KM) & Year

	M/S-TPL
	ADANI
	Adani Khavda Solar Project
	M/s. Jash Energy Pvt Ltd.
	Inspection of Manufacturing of Solar Project Equipment’s
	Galvanizing of Torque Tube-13, Tube Connector Upper & tube Connector Bottom Structure/Parts (Galvanization Testing-Mass of coating, Uniformity, Adhesion

	TUV RHEINLAND
	ADNOC
	China Petroleum Pipeline Engineering Company- Abu Dhabi
	Man Industries Ltd Anjar
	LSAW Bare Line Pipe Size – 48” (1219 mm) OD x 20.62 mm WT, & Spiral Bare Line Pipe Size – 48” (1219.0 mm OD X 14.50 mm WT 1219.0 mm OD X 17.48,20.32, & 23.63 API 5L L450M or X65M PSL2
	Raw material Inspection, WPS, PQT, Physical & Chemical Test, Dimensions Inspection, Hydro Test, NDT Testing & Pop pees, Daly Hydrogen crack Inspection etc. (Qty 116+10 KM Year 2023)

	Mein Hardt
	Rushmore Enterprises Inc
	Rush Pipe Line Project
	Surya Roshni Ltd Anjar
	6.625 MM OD X 5.56 MM WT, 12.75 MM OD X 6.02 MM WT , 4.5 MM OD X 5.56 MM WT, 8.625 MM OD X 5.56 MM WT,
	Raw material Inspection, WPS, PQT, Physical & Chemical Test, Dimensions Inspection, Hydro Test, NDT Testing & Pop pees, Daly Hydrogen crack Inspection etc.

	TUV RHEINLAND
	ADNOC
	China Petroleum Pipeline Engineering Company- Abu Dhabi
	Man Industries Ltd Anjar
	1219.0 mm OD X 14.50 mm WT 1219.0 mm OD X 17.48,20.32, & 23.63
	Raw material Inspection, WPS, PQT, Physical & Chemical Test, Dimensions Inspection, Hydro Test, NDT Testing & Pop pees, Daly Hydrogen crack Inspection etc.

	DNV
	Barossa Darwin Project
	Welspun crop ltd
	450SFD &450 SFDU
	34’’& 26’’OD X19.9/25.5 & 23.96 MM Wt
	Raw material Inspection, WPS, PQT, Physical & Chemical Test, Dimensions Inspection, Hydro Test, NDT Testing & Pop pees, Daly Hydrogen crack Inspection etc.

	KTI Middle Est Co LLC
	ADNOC (Onshore)
	JSW SAMAGOGA
	36”, (914 mm) OD X 15.8 mm WT X 5D Radius, IB 450 – PSL 2 (Sour Service)
	Hot Induction Bend R=5D, UG 90deg,69deg,22.5deg.57deg.45deg. 36” OD X 23.96 MM Wt
	Raw material Inspection, WPS, Welding PQT, Physical & Chemical Test, Dimensions Inspection, Hydro Test, NDT Testing ,(Qty 09 Nos Year 2022)



MAY 2021 – AUG 2021
Client: HRRL/EIL
EPCC-16 Mongla Crude Oil Pipeline and Associated Facilities
Vendor: JSIW Infrastructure Pvt. Ltd
Product: Size12.75” (323.90mmOD), 6.4 mm Wall (X-70M, PSL2) Thickness HFW & External Dual Layer Fusion Bonded Epoxy (FBE) Coating Pipes, Internally Bare
Performed raw material inspection, WPS, PQT, physical and chemical testing, dimensional inspection, hydro testing and NDT testing.
Performed coating raw material testing and inlet inspection of bare pipes.
Inspected coating application, epoxy and adhesive-coated pipes, 3LPE-coated pipes and final inspection.

Client: IOCL Dagoba / Guwahati Refinery
Anup Engineering
Vendor: UDHE
Product: Large Size Vertical Columns Dia. 2.5 Mtr(Max) Thickness 32 mm Length 60 Meters Max Material CS
Performed all-stage inspection, material identification, in-process inspection, final inspection, NDT, welding and painting inspection.

Client: KPCL Refinery
Ishan Equipment’s Pvt. Ltd
Vendor: KPCL
Product: Small to Medium Size Vessel and exchange, Material LTCS, CS & SS
Performed all-stage material identification and in-process inspection, final inspection, visual and dimensional inspection, hydrostatic and pneumatic testing, NDT, welding and painting inspection.

Client: MRPL/CDU VDU PROJECT
Anup Engineering
Vendor: Toyo Engineering
Product: Medium Size Heat Exchangers
Performed material identification, in-process inspection, final inspection, NDT, welding and painting inspection.

Client: Cryogenic liquid storage terminal, Jetty Pipeline Kandla
AEGIS Logistic
Vendor: TUVRHEINLAND
Product: API_5L_PSL2 X 70 M; 16’’ OD X 10.9 mm WT, 12’’ OD X 9.5 mm WT, 8’’ OD X 9.5 mm WT
Location: Kandla
Performed WPS, EQT, fit-up, welding, trenching, lowering, hydro testing, NDT testing and document checks.

Client: ADNOC P.J.S.C
Hail & Ghasha Development Project Package – 1 – Offshore Facilities
Vendor: NPCC-Saipem Joint Venture
Product: Site Fabricated Storage Tank & Shop Fabricated CS, SS Storage Tank
Inspected raw materials, WPS, welder qualifications, fit-up, welding, visual and dimensional inspection, hydro testing, pneumatic testing, NDT, final painting and documentation against approved drawings, ITPs and procedures.
Inspected storage tanks including GH5161TK102 Utility Water Storage Tank, GH5173-TK101 Firewater Storage Tank, GH5126-TK101 Off Spec. Condensate/Oils Tank and HL0369-TK101 Diesel Storage Tanks.

JAN 2025 – JAN 2026
Client: HIGH VIEW POWER
AIR ENERGY STORAGE CRYOGENIC VESSEL
Vendor: DNV
Product: 5800 DIA. X 41 METER LONG, SA312 TP 304 material, 5 Nos. quantity
Position: Inspection Engineer Surveyor
Performed material identification and in-process inspection as per drawings.
Performed fit-up, final, visual and dimensional inspection, hydrostatic and pneumatic testing, NDT, welding and painting inspection.

2025
Client: CPC TAIWAN Project
36” OD 228 KM LSAW coated steel pipe and bare pipe procurement
Vendor: Man Industries (India) Ltd., Anjar
Product: 36” OD LSAW DNV SAWL F, D coated steel pipe and bare pipe
Location: Anjar, Gujarat
Inspected bare pipe and coating production for the 36-inch OD LSAW pipe procurement project.

2025
Client: NPCC, Maximize Ethane Recovery & Monetization (MERAM)-EPC
36” & 42”, 48” OD LSAW pipe inspection
Vendor: Ratnamani Metals and Tubes Ltd., India
Product: ASTM A672 Gr. C60 CL22 NACE pipe
Inspected LSAW pipe manufacturing and associated quality activities.

2025
Client: ESTIDAMA Sales Gas Pipeline Network Enhancement Project, Packages 4 and 7
Shuwaib Sajaa Pipeline and Margham Pipeline
Vendor: Jindal SAW Ltd., Mundra
Product: 30-inch and 48-inch OD LSAW bare pipe, internal and external coating, hot induction bends and coated hot induction bends
Location: Mundra, Gujarat
Inspected 230 km of LSAW bare pipe, internal and external coating, hot induction bends and hot induction bend coating.

2024 – 2025
Client: ADNOC
ADNOC EPC Works for Wave C3A Petrojet Project
Vendor: Jindal SAW Ltd., Mundra
Product: 142 km LSAW bare pipe, API 5L L450MS (X65MS) and L415MS (X65MS), PSL-2
Location: Mundra, Gujarat
Inspected pipe manufacturing, material identification, in-process and final inspection, NDT, welding and painting/coating activities.

2024
Client: ADNOC-OFFSHORE / NPCC
ADNOC Offshore Project
Vendor: Jindal SAW Ltd., Mundra
Product: 160 km LSAW bare pipe and 3LPE coating, Grade X70M PSL-2
Location: Mundra, Gujarat
Inspected LSAW bare pipe and 3LPE coating production.

2023 – 2024
Client: Qatar Gas Pipeline Project
D7519-NFPS Project-Offshore Comp1
Vendor: Welspun Corp Ltd., Anjar
Product: 131 hot induction bends, 822.34 OD x 26.97 mm WT, 5D radius
Location: Anjar, Gujarat
Inspected manufacturing and testing of hot induction bends.

2023
Client: ADANI
Adani Khavda Solar Project
Vendor: Jash Energy Pvt. Ltd.; Adani
Product: Solar project equipment and galvanized torque tube, tube connector upper and tube connector bottom structures/parts
Location: Khavda
Inspected solar project equipment manufacturing and galvanized coating.
Performed galvanizing tests including mass of coating, uniformity and adhesion.

2023
Client: China Petroleum Pipeline Engineering Company
China Petroleum Pipeline Project
Vendor: Man Industries India Ltd., Anjar
Product: 180 km LSAW bare pipe and 3LPE coating, Grade X65M PSL-2
Location: Anjar, Gujarat
Inspected LSAW bare pipe and 3LPE coating production.

2022 – 2023
Client: Rush Pipe Line Project
Rush Pipe Line Project
Vendor: Surya Roshni Ltd., Anjar
Product: 98 km HFW bare pipe and 3LPE coating, Grade X65 PSL-2
Location: Anjar, Gujarat
Inspected ERW/HFW pipe manufacturing and 3LPE coating.

2022
Client: MRPL/CDU VDU PROJECT
MRPL/CDU VDU Project
Vendor: Praj Industries Pvt. Ltd., Gandhi Dham
Product: Small to medium vessels and exchangers, LTCS, CS and SS
Location: Gandhi Dham, Gujarat
Inspected 24 jobs including suction volume bottles and discharge volume bottles.
Performed material identification, in-process, final, visual and dimensional inspection, hydrostatic and pneumatic testing, NDT, welding and painting inspection.

2022
Client: KPCL Refinery
KPCL Refinery Project
Vendor: Ishan Equipment’s Pvt. Ltd.
Product: Small to medium vessels and exchangers, LTCS, CS and SS
Performed all-stage inspection, material identification, final, visual and dimensional inspection, hydrostatic and pneumatic testing, NDT, welding and painting inspection.

2022
Client: IOCL Dagoba / Guwahati Refinery
IOCL Dagoba / Guwahati Refinery
Vendor: Anup Engineering
Product: Large vertical columns, CS, shell SA 516 Gr. 60 and Gr. 70
Inspected large vertical columns up to 2.5 m diameter, 32 mm thickness and 60 m length.
Performed material identification, in-process, final, NDT, welding and painting inspection.

2022
Client: GAIL & IOCL
Cryogenic Liquid Storage Terminal Jetty Pipeline Project
Vendor: AEGIS Logistic Ltd., Kandla
Product: 15 km line pipe, 16-inch, 12-inch and 8-inch OD, Grade X70M and X65M PSL-2
Location: Kandla, Gujarat
Inspected line pipe work, WPS, EQT, fit-up, welding, trenching, lowering, hydro testing, NDT and documentation.

2021 – 2022
Client: Barossa Project
Barossa Project
Vendor: Welspun Corp Ltd., Anjar
Product: 220 km LSAW bare pipe, Grade 450 SFD and 450 SFDU, 26-inch OD
Location: Anjar, Gujarat
Inspected LSAW bare pipe manufacturing and associated testing.

2021
Client: Baker Hughes
Baker Hughes Project
Vendor: Praj Industries
Product: Suction volume bottle, discharge volume bottle and recovery tank
Performed all-stage inspection, material identification, final, visual and dimensional inspection, hydrostatic and pneumatic testing, NDT, welding and painting inspection.

2021
Client: IGL Rajasthan Project
IGL Rajasthan Project
Vendor: Surya Roshni Ltd., Anjar
Product: 190 km HFW bare pipe and 3LPE coating, Grade X56 PSL-2
Location: Anjar, Gujarat
Inspected ERW/HFW bare pipe and 3LPE coating.

2020 – 2021
Client: Public Authority of Water, Sultanate of Oman
Reinforcement of AD Dahlia Water Transmission System – Phase II
Vendor: L&T
Product: 148 km submerged arc helical welded pipe, 32-inch to 68-inch, API 5L L360 PSL-1, external 3LPE and internal liquid paint coating
Location: Sultanate of Oman
Performed raw material inspection, WPS, PQT, physical and chemical testing, dimensional inspection, hydro testing and NDT testing.
Performed coating raw material testing, inlet inspection of bare pipes, coating application inspection, epoxy/adhesive and 3LPE-coated pipe testing and final inspection.

2019 – 2020
Client: GIGL
Mehsana-Bhatinda Pipeline Project (Natural Gas Pipeline)
Vendor: JSIW Infrastructure Pvt. Ltd.
Product: 252 km submerged arc helical welded pipe, 30-inch and 18-inch OD, API 5L L485M PSL-2, external 3LPE and internal liquid paint coating
Inspected raw materials, WPS, PQT, physical and chemical testing, dimensions, hydro testing and NDT.
Inspected coating raw materials, bare pipe inlet, coating application, epoxy/adhesive and 3LPE-coated pipes and final inspection.

2019
Client: IOCL
IOCL Pipeline Project
Vendor: Man Industries India Ltd., Anjar
Product: 265 km HSAW and LSAW bare pipe and 3LPE coating, Grade X70M PSL-2
Location: Anjar, Gujarat
Inspected HSAW/LSAW pipe manufacturing and 3LPE coating.

2019
Client: GAIL, KKBMPL, Phase II
GAIL PL.0103 / PL.0104 Ahmednagar & Aurangabad Gas Pipeline
Vendor: Man Industries India Ltd., Anjar
Product: 170 km HSAW and LSAW bare pipe and 3LPE coating, Grade X65M PSL-2
Location: Anjar, Gujarat
Inspected HSAW/LSAW pipe manufacturing and 3LPE coating.

2019
Client: SAIPAM Project
SAIPAM Project
Vendor: Jindal SAW Ltd., Mundra
Product: 180 km LSAW bare pipe and 3LPE coating, Grade X70M PSL-2
Location: Mundra, Gujarat
Inspected LSAW bare pipe and 3LPE coating production.

2018 – 2019
Client: ENI East Spingarn Me Rakes Development Project
ENI East Spingarn Me Rakes Development Project
Vendor: Welspun Corp Ltd., Dahaj
Product: 300 km LSAW bare pipe, ISO 3183 L450 MO
Location: Dahaj, Gujarat
Inspected LSAW bare pipe manufacturing and testing.

2018
Client: IOCL
IOCL Paradeep to Haldia Pipeline
Vendor: Jindal SAW Ltd., Mundra
Product: 260 km LSAW bare pipe and 3LPE coating, Grade X70M PSL-2
Location: Mundra, Gujarat
Inspected LSAW bare pipe and 3LPE coating production.

PLAQUEMINES LNG Project

Ruwais LNG Project
Vendor: TJN (JV) - Technip Energies
Product: Liquid Nitrogen Storage and Vaporisation

Client: ADNOC
Hail & Ghasha Development Project Package 2 - Onshore Facilities
Vendor: M/s. Cunado Middle East for Pipes and Valves, L.L.C. (Tecnimont)
Product: Pipes and valves
Location: Abu Dhabi

Client: ADNOC
Hail & Ghasha Development Project Package 1 – Offshore Facilities
Vendor: NPCC-Saipem Joint Venture
Location: Abu Dhabi

JSIW Infrastructure Pvt. Ltd.

IOCL Dagoba / Guwahati Refinery

IOCL KGPL Project

IOCL O&M City Gas Distribution Pipe Line

MRPL/CDU VDU Project

ONGC PRP-6/VML Project

Public Authority of Water (PAW) of Sultanate of Oman Project

Zubair Oil Field Development Project

Laying of 42” OD Submarine Pipeline and Installation of No. SPM System in Gulf of Kutch off Vadinar, Gujarat IOCL Project
Location: Gulf of Kutch, Vadinar, Gujarat

Trans Canada Pipe Line Project (TCPL)
Location: Canada

L&T Pipe Line Project

Indraprastha Gas Limited Project

KPCL Refinery Project

GAIL PL.0112 SAPL-SEC-III Pipeline Project

EPCM Services COT at Paradip, PNCPL & NSPPL (NRL Plate Inspection)
Location: Paradip

Kalamanga-Paradip Iron Ore Slurry Pipeline Project

Renew-Envision 3.3MW_156RD_140HH for RTC W2 Projects
Location: Kurudhagi, Karnataka

Mundra Solar Energy Project
Location: Mundra

Client: M/s Oil SERV
SS Pipes & Tube Inspection
Vendor: Venus Pipes and Tubes Limited
Product: SS pipes and tubes, Grade TP 316/316L
Reviewed RMTC, raw material testing, heat treatment, mechanical and chemical testing and hydrostatic testing.
Performed pipe dimensional inspection of outside diameter, wall thickness and length as per QAP.

Client: M/s ADNOC
SS Pipes & Tube Inspection
Vendor: Venus Pipes and Tubes Limited
Product: SS pipes and tubes, Grade TP 316/316L
Reviewed RMTC, raw material testing, heat treatment, mechanical and chemical testing and hydrostatic testing.
Performed pipe dimensional inspection of outside diameter, wall thickness and length as per QAP.

Client: Petroleum Development Oman
Dhiab Infill Development
Vendor: Ratnamani Metals and Tubes
Product: SS tube, ASTM A358 TP316/316L Class 1
Location: Oman
Reviewed RMTC, raw material testing, heat treatment, mechanical and chemical testing and hydrostatic testing at 1000 PSIG.
Performed dimensional and visual inspection and confirmed pipes were within range and free from cracks, sweats, leaks and injurious surface defects.

SKILLS
QA/QC Management
Third-Party Inspection
Steel Pipe and Tube Inspection
Welding Inspection
NDT Inspection
Coating / Painting Inspection
Pressure Vessel Inspection
Heat Exchanger Inspection
Pipeline Inspection
Vendor Inspection
Expediting
WPS / PQR / WPQR Review
Quality Plan and ITP Review
Welder Qualification
Radiograph Interpretation
Material Traceability
Quality Documentation
Client and TPI Coordination

COMMODITIES
Steel Pipes
ERW Pipes
HFW Pipes
HSAW Pipes
LSAW Pipes
Hot Induction Bends
Piping
Pipe Fittings
Flanges
Valves
Pressure Vessels
Heat Exchangers
Storage Tanks
Columns
Reactors
Boilers
Steam Drums
Tube Sheets
Tubes
Tube Bundles
Baffles
Skids
Structural Steel
Plates
Coils
Forgings
Welding Consumables
Coating Material
Concrete Weight Coating
Solar Project Equipment
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