
ANDY DU

SUMMARY
Andy Du has 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has worked on major projects and coordinated effectively between contractors and clients. His inspection scope covers pressure vessels, packages and skids, gas turbine cylinders, dynamic equipment, subsea products, piping, valves, steel plates and forgings, chains, containers, cranes, bridges, and other equipment. Andy has extensive knowledge of international and national standards and welding processes including SAW, SMAW, GTAW, FCAW, and GMAW. He also has specialist coating inspection experience covering surface preparation, blasting, paint application, DFT, curing, repairs, and adhesion.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS, ASME, ASTM, API, GB, HB, JB, EN, ISO…

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed resident, mechanical, coating, subsea, and third-party inspection across pressure vessels, packages and skids, FPSO-related equipment, piping, valves, steel structures, cranes, bridges, containers, and other products.
Inspected raw materials, fabrication, fit-up and welding, NDT, pressure and performance testing, dimensions, visual quality, coating, assembly, FAT, final inspection, packing, and preservation.
Reviewed MTRs, ITPs, WPS/PQRs, welder qualifications, NDT records, certificates, manufacturing documentation, and MRB dossiers.
Coordinated inspection activities between contractors, manufacturers, clients, end users, and suppliers on major projects.

PROJECTS

Client: TEN (End user Total)
GRANMORGU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Performed painting inspection.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd..
Product: AGC Package -Separator
Position: Mechanical inspector
Performed raw material inspection, including flange, elbow, and forging inspection.
Monitored clad welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Performed visual inspection.
Inspected clad thickness.
Witnessed NDT.
Witnessed PMI testing.
Reviewed documents.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualifications, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Performed painting inspection.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed chemical analysis of cladding.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Monitored the welding process.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Monitored welding processes as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak testing and hydrostatic testing.
Inspected pickling, passivation, blasting, and painting.
Verified nameplates.
Performed final inspection.
Inspected marking and packing.
Reviewed MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected material cutting and traceability.
Inspected fit-up and tack welding.
Monitored welding processes as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness testing.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak testing and hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected material cutting and traceability.
Inspected fit-up and tack welding.
Monitored welding processes as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness testing.
Performed PWHT inspection.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed air-tight leak testing and hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Performed raw material inspection.
Inspected formed heads.
Inspected fit-up and tack welding.
Monitored welding processes.
Performed visual inspection after welding.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed dimensional and visual inspection.
Inspected heat treatment.
Witnessed hydrostatic testing.
Inspected blasting and painting.
Performed final inspection.
Inspected package shipping and preservation.
Reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Performed raw material inspection.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed cleanliness inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Performed raw material inspection.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Witnessed helium and nitrogen leakage testing.
Performed final inspection.
Inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management inspection.
Performed mechanical completion checks.
Witnessed FAT testing.
Performed final inspection.
Inspected package shipping and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspector
Monitored feed gas heater fabrication.
Monitored membrane housing fabrication.
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT testing.
Performed final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT testing and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Performed vessel fabrication inspection.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspector
Performed raw material inspection, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Witnessed NDE testing.
Performed dimensional inspection.
Witnessed hydrostatic testing.
Performed blasting and painting inspection.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management.
Performed mechanical completion checks.
Inspected insulation.
Witnessed FAT and system leak testing.
Performed weighing and COG inspection.
Performed final inspection.
Inspected package shipping and preservation.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspector
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Performed parts machining quality inspection.
Inspected fit-up and welding.
Witnessed function, vibration, and noise testing.
Inspected package shipping and preservation.
Reviewed documents.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Witnessed CPT testing.
Inspected outside surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Inspected outside surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected coating system qualification.
Inspected paint and coating materials.
Inspected outside surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed documents.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected pickling and passivation.
Inspected coating system qualification.
Inspected paint and coating materials.
Inspected surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Inspected outside surface cleanliness before blasting.
Inspected abrasive and compressed air.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDemott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP Coating inspector
Reviewed documents.
Inspected paint and coating materials.
Inspected surface cleanliness before blasting.
Inspected environmental conditions, including air temperature, surface temperature, humidity, and dew point.
Inspected abrasive and compressed air.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint type mixing and thinning.
Inspected wet film thickness and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Performed pull-off and crosscut adhesion inspection.

Client: Jiangnan Boiler &Pressure vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler &Pressure vessel
Position: NACE CIP coating inspector
Reviewed documents.
Performed cleanliness checks after blasting, including cleanliness degree, roughness, and dust.
Inspected curing.
Performed visual examination and DFT inspection for each layer.
Inspected paint repairs.
Performed crosscut adhesion inspection.
Performed final and marking inspection.

Client: Baker Hughes
Product in XT system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Tree frame, Protection structure, Debris cap, Debris Canopy Shipping Skid
Performed raw material inspection, including MTR review and raw material receipt inspection.
Inspected material cutting and marking.
Performed machining inspection.
Witnessed fit-up and monitored welding on structures.
Witnessed UT and MT of welds.
Performed visual inspection of welds.
Verified base-frame dimensions.
Inspected coating surface preparation and painting.
Performed adhesion and holiday testing.
Performed assembly inspection.
Witnessed FAT testing.
Performed final inspection.
Reviewed MRB documentation.
Inspected package and shipping.

Client: Baker Hughes
Product in Connections system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Clamp connectors (VCCS &HCCS Type T, HCCS-L, Test Clamp), Pressure Caps, Vent caps, Light Duty Clamps
Performed raw material inspection.
Performed machining inspection.
Inspected NDT before clad welding.
Monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT.
Witnessed hardness testing.
Performed dimensional inspection.
Performed load test and inspection.
Inspected blasting and painting.
Performed adhesion and holiday testing.
Performed assembly inspection.
Witnessed FAT, including weight, visual, electrical continuity, and COG testing.
Performed final inspection.
Reviewed MRB documentation.
Inspected package and shipping.

Client: Baker Hughes
Product in GFDS System
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Porch, Termination, Male Hub/pup-piece
Performed raw material inspection.
Performed machining inspection.
Inspected NDT before clad welding.
Monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT.
Performed dimensional inspection.
Witnessed hydrostatic and gas testing.
Inspected blasting and painting.
Performed assembly inspection.
Witnessed FAT, including weight, visual, electrical continuity, and back seal testing.
Performed final inspection.
Reviewed MRB documentation.
Inspected package and shipping.

Client: KOC, Eurobas Piping, Kim Seng Huat Hardware, S. de RL Arendal de C.V, Sam Lain Equipment Services Pte Ltd, Ruicheng
Pipe & tube
Vendor: Yangzhou Lontrin, Tianjing TPCO, Jiangsu Valin-Xigang, Wuxi Dexing, Chengdu Pangang group, Zhejiang Jiuli Hi-Tech Metals, Panyu Chu Kong Steel pipe, Hengyang Valin, East China Power Station, Jiangyin City Changjiang Steel pipe Co
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Position: Third party inspection & Certification
Performed manufacturing procedure qualification testing.
Performed product chemical analysis and mechanical property testing.
Witnessed hydrostatic testing.
Witnessed NDT testing, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Standards: ASME B16.5 ASME B16.9, ASME B16.11, MSS SP-97
Position: Third party inspection & Certification
Reviewed documents.
Performed product chemical analysis and mechanical property testing.
Witnessed hardness testing.
Witnessed PMI testing.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Position: Third party inspection & Certification
Reviewed documents.
Witnessed PMI, mechanical property, and hardness testing.
Witnessed NDT, including PT, MT, UT, and RT.
Performed assembly inspection.
Performed visual and dimensional inspection.
Witnessed pressure testing, including hydraulic, shell, seat, backseat, low-pressure gas, and operation testing.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Product: SubSurface Safety Valve & Packer
Standards: API 14A, API 11D
Position: Third party inspection & Certification
Reviewed documents.
Witnessed drift testing.
Witnessed function inspection.
Performed dimensional and visual inspection.
Performed marking inspection.
Inspected coating and protection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed hardness testing.
Witnessed UT and MT.
Performed visual and dimensional inspection.
Inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed proof-load and break-load testing.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Position: Third party inspection & Certification
Reviewed documents.
Monitored casing.
Witnessed chemical and electrochemical analysis.
Performed crosscut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Position: Third party inspection & Certification
Reviewed documents.
Witnessed hydrostatic, performance, and break-load testing.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Experience in construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Container
Reviewed documents.
Performed floorboard and corner-fitting sampling.
Witnessed relevant testing.
Performed routing inspection covering welding processes, assembly, and dimensions.
Performed visual quality inspection after welding.
Performed coating inspection.
Witnessed general prototype testing.
Performed whole-container inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Experience in construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Reviewed related documents and procedures, including WPS, welder qualifications, and drawings.
Performed raw material re-inspection.
Inspected main structural steel assembly.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Performed structural final inspection.
Performed coating inspection.
Witnessed FAT and EFAT of cranes.

Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Product: Steel bridge
Position: CWI inspector
Performed raw material re-inspection.
Witnessed mechanical property testing and product chemical analysis for steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Checked zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Experience in the construction of Equipment
Product: Gland Condenser & Handing Clamp
Reviewed quality control documents, including ITP, WPS/PQR, WQT, and NDT.
Reviewed material and equipment calibration and consumable certificates.
Witnessed hydrostatic testing.
Witnessed cleaning and dry checks.
Witnessed surface preparation.
Performed visual and dry film checks.
Inspected rust prevention, including VCI application inside the gland condenser.
Performed visual and dimensional inspection, including nameplates.
Inspected packing and marking.
Reviewed manufacturing final inspection.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Steel Structure Inspection
Welding Inspection
Third-Party Inspection
Pressure Vessel Inspection
Mechanical Inspection
Subsea Product Inspection
FPSO Topside Inspection
Coating Inspection
NDT Inspection
Package and Skid Inspection
Crane and Heavy Lifting Equipment Inspection
Bridge Inspection
Quality Control Document Review
Contractor and Client Coordination

COMMODITIES
Coating Material
Pressure Vessels
FPSO Topsides
Subsea Structures
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridge Steel
Steel Plates
Forgings
Gas Turbine Cylinders
Packages and Skids
Pumps
Membrane Housings
Heat Exchangers
Separators
Scrubbers
Cranes
Containers
Ropes
Anodes
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