
ANDY DU

SUMMARY
Andy Du is an inspector with 14 years of experience in material inspection, steel structure fabrication, FPSO topside inspection, subsea structures monitoring, crane monitoring, pressure vessels, and third-party inspection. He has performed resident and mechanical inspection on pressure vessels, FPSO packages, skids, gas turbine cylinders, dynamic equipment, and heavy lifting equipment for major projects and clients including TEN, Sinopec, Veolia, SLB, CNOOC, Air Liquide, and Modec. Andy has extensive welding-process experience covering SAW, SMAW, GTAW, FCAW, and GMAW, together with broad knowledge of international and national standards. He is experienced in coating inspection, subsea products, pipes, fittings, valves, forgings, chains, bridges, and containers. He also brings strong coordination ability between contractors and clients on large projects.

EDUCATION
2005~2008 University: Nanjing University of Technology

QUALIFICATIONS AND TRAINING
2008: Training for CWI
2012: Training for Nace Coating Level II
2022: Training for UT/MT
NACE CIP Level II
CWI Certificate
ASNT UT level 2 certificate
ASNT MT level 2 certificate

CODES AND STANDARDS
AWS
ASME
ASTM
API
GB
HB
JB
EN
ISO…

WORK EXPERIENCE

FREELANCE (VARIOUS CLIENTS)
Performed material, mechanical, pressure vessel, FPSO package, subsea product, coating, welding, and third-party inspection across major industrial projects.
Coordinated inspection activities between contractors, manufacturers, clients, and end users.
Reviewed quality documents, inspection and test plans, welding documentation, certificates, and manufacturing record books.
Inspected steel structures, piping, valves, skids, cranes, bridges, containers, and other equipment through fabrication, testing, final inspection, and shipment.

PROJECTS

Client: TEN (End user Total)
GRANMORGU PROJECT (Block 58) Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Misc Vessels (NITROGEN RECEIVER/HEATING MEDIUM EXPANSION VESSEL/COOLING MEDIUM EXPANSION VESSEL/Desulfated Water Buffer Vessel/Corrosion Inhibitor Buffer Vessel/Asphaltene Inhibitor Buffer Vessel/Methanol Buffer Vessel/COOLING MEDIUM EXPANSION VESSEL (ESSENTIAL)/ DEAD OIL BUFFER VESSEL/STARBOARD CLOSED DRAIN VESSEL/PORTSIDE CLOSED DRAIN VESSEL/LABORATORY DRAIN TANK/Menthol Recycle Cooler )
Position: Resident inspector
Inspected raw materials, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Inspected painting.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Sinopec (End user Total)
TILENGA Project
Vendor: Shandong Kerui Petroleum & Gas Equipment Co., Ltd.
Product: AGC Package -Separator
Position: Mechanical inspector
Inspected raw materials, including flanges, elbows, and forgings.
Monitored the clad welding process, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Performed visual inspection.
Inspected clad thickness.
Witnessed NDT.
Witnessed PMI testing.
Reviewed documents.

Client: Veolia (End AIR Products)
VEOLIA Darrow Blue Energy Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Vessels (TEG Contactor/TEG Flash Drum/Rich TEG Filter/TEG Carbon Filter/TEG Stripping Column/TEG Surge Drum/Waste Water Column /Steam Condensate KO Drum /Compressor Suction KO Drum/Lean / Rich TEG Exchanger//TEG Still Column/TEG Reboiler)
Position: Resident inspector
Inspected raw materials, including MTR review and raw material receipt inspection.
Inspected formed heads.
Inspected fit-up and tack welding, including gap, alignment, and cleanliness.
Monitored welding processes, including preheat, weld consumables, welding parameters, welder qualification, and protection.
Inspected marking and openings.
Inspected nozzle fit-up and welding to shells and heads.
Witnessed NDT.
Inspected pressure vessel internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Inspected painting.
Verified nameplates.
Witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Chervon)
VEOLIA Gorgon PWT Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: DESANDING HYDROCYCLONES, DEOILING HYDROCYCLONES, SANDING ACCUMULATOR
Position: Resident inspector
Inspected raw materials, including MTR review and receipt inspection.
Inspected formed heads, fit-up, tack welding, marking, and openings.
Inspected nozzle fit-up and welding to shells and heads.
Performed chemical analysis of cladding.
Witnessed NDT.
Inspected internal cleaning.
Performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates and witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
Western Surat Gas Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol Dehydration Vessel
Position: Resident inspector
Inspected raw materials, including MTR review and receipt inspection.
Inspected formed heads, fit-up, tack welding, marking, and openings.
Monitored welding processes and inspected nozzle fit-up and welding to shells and heads.
Inspected PWHT and witnessed NDT.
Inspected internal cleaning and performed visual and dimensional inspection.
Witnessed hydrostatic testing.
Inspected pickling and passivation treatment.
Verified nameplates and witnessed weighing tests.
Inspected marking and packing.
Reviewed MRB documentation.

Client: Veolia (End user Senex)
SENEX-MIMAS Compression Facility Phase A Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Glycol vessels
Position: Resident inspector
Inspected raw materials, formed heads, fit-up, tack welding, marking, and openings.
Monitored welding as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected nozzle fit-up and welding to shells and heads.
Inspected PWHT and witnessed NDT.
Inspected internal cleaning and performed visual and dimensional inspection.
Witnessed air-tight leak and hydrostatic tests.
Inspected pickling, passivation, blasting, and painting.
Verified nameplates, performed final inspection, and witnessed weighing.
Inspected marking and packing.
Reviewed MRB documentation.

Client: SLB (End user OTC)
SAKARYA GAS FIELD DEVELOPMENT project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Vessels; TEG Vessels, TEG Exchangers
Position: Resident inspector
Inspected raw materials, formed heads, material cutting, and traceability.
Inspected fit-up and tack welding.
Monitored welding as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, and nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness tests, PWHT, and NDT.
Inspected internal cleaning and performed visual and dimensional inspection.
Witnessed air-tight leak, hydrostatic, and weighing tests.
Inspected pickling, passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Modec)
Marlim 1 (FPSO Anita Garibaldi) project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: PWT Vessels; Oil Vessels, TEG Vessels, Amine Vessels
Position: Resident inspector
Inspected raw materials, formed heads, material cutting, and traceability.
Inspected fit-up and tack welding.
Monitored welding as per WPS and PQR for GTAW, FCAW, SMAW, SAW, and overlay welding.
Inspected marking, openings, and nozzle fit-up and welding to shells and heads.
Witnessed PMI and hardness tests, PWHT, and NDT.
Inspected internal cleaning and performed visual and dimensional inspection.
Witnessed air-tight leak, hydrostatic, and weighing tests.
Inspected pickling, passivation, nameplates, marking, and packing.
Reviewed MRB documentation.

Client: SLB (End user Woodside)
SNE project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Exchangers; TEG Vessels, Amine Vessels, Amine Exchangers
Position: Resident inspector
Inspected raw materials and formed heads.
Inspected fit-up and tack welding and monitored welding processes.
Performed visual inspection after welding.
Inspected marking, openings, and nozzle fit-up and welding to shells and heads.
Performed dimensional and visual inspection and heat treatment inspection.
Witnessed hydrostatic testing.
Inspected blasting, painting, final inspection, package shipping, and preservation.
Reviewed MRB documentation.

Client: CNOOC
CNOOC Shenzhen Power Plant Upgrade Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas turbine intake cylinder and gas turbine exhaust cylinder
Position: Mechanical inspector
Inspected raw materials.
Performed dimensional and visual inspection.
Witnessed hydrostatic testing.
Performed cleanliness inspection and final inspection.
Inspected package shipping and preservation.

Client: H2 Green Steel
SC00039793 H2 Green Steel Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Cylinder (Ferritic ductile cast iron ASTM A 395)
Position: Mechanical inspector
Inspected raw materials.
Performed dimensional and visual inspection.
Witnessed hydrostatic and helium/nitrogen leakage tests.
Performed final inspection.
Inspected package shipping and preservation.

Client: Seatrim
FPSO P83, Buzios Project
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: RECIRCULATION PUMP SKID
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, and lifting lugs.
Monitored piping spool fabrication.
Performed dimensional and visual inspection and witnessed hydrostatic testing.
Inspected blasting and painting.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management inspection and mechanical completion checks.
Witnessed FAT testing.
Performed final inspection and inspected package shipping and preservation.

Client: Air Liquide
PORTHOS PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEMBRANE SKID
Position: Resident inspection
Monitored feed gas heater and membrane housing fabrication.
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spools.
Witnessed NDE and hydrostatic testing.
Performed dimensional and visual inspection.
Inspected blasting, painting, insulation, and flange management.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed mechanical completion checks, witnessed FAT, and performed final inspection.

Client: Sinopec (End User Total)
TILENGA PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: POLYMER TEST SEPARATOR Package
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing.
Performed dimensional and visual inspection and inspected blasting, painting, and insulation.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Witnessed FAT and system leak tests.
Performed weighing and COG inspection, final inspection, and package shipping and preservation.

Client: Veolia (End User: Air Products)
Edmonton Net Zero Hydrogen Energy Complex
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Skid
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Performed vessel fabrication inspection.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing.
Performed dimensional inspection and inspected blasting, painting, and insulation.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Witnessed FAT and system leak tests.
Performed weighing and COG inspection and final inspection.

Client: SLB
SAKARYA GAS FIELD DEVELOPMENT PROJECT
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: MEG Skid and TEG Skid
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing.
Performed dimensional inspection and inspected blasting, painting, and insulation.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Witnessed FAT and system leak tests.
Performed weighing and COG inspection, final inspection, package shipping, and preservation.

Client: Modec
SNE project (FPSO Woodside)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: TEG Regeneration System
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing.
Performed dimensional inspection and inspected blasting, painting, and insulation.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Witnessed FAT and system leak tests.
Performed weighing and COG inspection, final inspection, package shipping, and preservation.

Client: Modec
Carcara project (Bacalhau FPSO)
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Gas Dehydration and TEG Regeneration System
Position: Resident inspection
Inspected raw materials, including structure, piping, valves, and piping fittings.
Monitored primary and secondary structure fabrication, monorails, lifting lugs, and piping spool fabrication.
Witnessed NDE and hydrostatic testing.
Performed dimensional inspection and inspected blasting, painting, and insulation.
Monitored structure, piping spool, valve, and other free-issue installation.
Performed flange management and mechanical completion checks.
Witnessed FAT and system leak tests.
Performed weighing and COG inspection and final inspection.

Phase II of the 2×660MW Coal-Fired Power Plant Project along the Coast of Vietnam
Vendor: Zhejiang Zifeng Technology Co., Ltd.
Product: Main plant building explosion-proof roof fan
Position: Resident inspection
Location: Vietnam
Performed centrifugal machine and motor incoming inspection.
Inspected free-issue materials, including MTCs, certificates, and test reports.
Inspected parts machining quality.
Performed fit-up and welding inspection.
Witnessed function, vibration, and noise tests.
Inspected package shipping and preservation.
Reviewed documents.

Client: HHI
Trion Project
Vendor: Himile Mechanical Manufacturing
Product: PWT Vessels, SWT Vessel, Oil Vessel, Piping
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected outside surface cleanliness before blasting, abrasive, and compressed air.
Inspected environmental conditions including air temperature, surface temperature, humidity, and dew point.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual examination and DFT inspection.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: SBM
Whiptail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers, Pipings
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface preparation, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection.
Inspected paint repair and adhesion by pull-off and crosscut testing.

Seawater Filter Package
Vendor: Himile Mechanical Manufacturing
Position: NACE CIP Coating inspector
Reviewed documents and coating-system qualification.
Inspected paint and coating materials, surface preparation, abrasive, and compressed air.
Inspected environmental conditions before blasting.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection.
Inspected paint repair and adhesion by pull-off and crosscut testing.

Client: Hitachi
FPSO P-80 Buzios Project
Vendor: Himile Mechanical Manufacturing
Product: Fresh Water Maker for Oil Dilution (RO Skid)
Position: NACE CIP Coating inspector
Reviewed documents.
Performed visual examination and DFT inspection.
Inspected paint repairs.
Inspected adhesion by pull-off and crosscut testing.

Client: SBM
ALMIRANTE FPSO
Vendor: Himile Mechanical Manufacturing
Product: CO2 Removal Membrane Skid, Separator Oil Vessels, Vessel Misc. Pressure, Scrubber Vessels Gas
Position: NACE CIP Coating inspector
Reviewed documents and inspected pickling and passivation.
Inspected coating-system qualification and paint and coating materials.
Inspected surface preparation, abrasive, compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: SBM
Yellowtail Project
Vendor: Himile Mechanical Manufacturing
Product: TEG Skid, TEG Vessels, TEG Exchanger, Separators, Scrubbers, Exchangers
Position: NACE CIP Coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface preparation, abrasive and compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: JGC
WHRU, Pressure Vessels
Vendor: Himile Mechanical Manufacturing, Alfa Laval (Qingdao), Qingdao McDermott Wuchuan
Product: Pressure Vessel - Rich MEG Separator, Hydrocarbon Removal Vessel, MEG Regeneration Column, Reflux Drum, Flash Separator, Downcomer, Reclaimer KO Drum, Calcium Removal Vessel, Salt Vessel, Centrate Buffer Vessel, CIP Tank, CIP Skid, WHRU – Stack, Outlet Duct, Inlet Duct, By-pass, External of seal air Duct
Position: NACE CIP coating inspector
Reviewed documents and inspected paint and coating materials.
Inspected surface preparation, abrasive, compressed air, and environmental conditions.
Inspected blasting cleanliness, roughness, dust, and soluble salts.
Inspected paint mixing and thinning, wet film thickness, and curing.
Performed visual and DFT inspection.
Inspected paint repairs and adhesion by pull-off and crosscut testing.

Client: Jiangnan Boiler & Pressure Vessel
Waste Heat Boiler
Vendor: Jiangnan Boiler & Pressure Vessel
Position: NACE CIP coating inspector
Reviewed documents.
Checked cleanliness after blasting, including cleanliness degree, roughness, and dust.
Inspected curing and visual examination and DFT for each layer.
Inspected paint repairs and adhesion by crosscut testing.
Performed final and marking inspection.

Client: Baker Hughes
Product in XT system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Tree frame, Protection structure, Debris cap, Debris Canopy, Shipping Skid
Position: Inspector
Inspected raw materials, including MTR review and receipt inspection.
Inspected material cutting and marking.
Performed machining inspection.
Witnessed fit-up and monitored structural welding.
Witnessed UT and MT of welds and performed visual weld inspection.
Verified base-frame dimensions.
Inspected coating surface preparation, painting, adhesion, and holiday testing.
Performed assembly and FAT inspection.
Performed final inspection, MRB review, and package and shipping inspection.

Client: Baker Hughes
Product in Connections system
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Clamp connectors (VCCS &HCCS Type T, HCCS-L, Test Clamp), Pressure Caps, Vent caps, Light Duty Clamps
Position: Inspector
Inspected raw materials and machining.
Inspected NDT before clad welding and monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT.
Witnessed hardness, dimensional, load, and painting inspections.
Inspected blasting, adhesion, holiday testing, and assembly.
Witnessed FAT, including weight, visual, electrical continuity, and COG tests.
Performed final inspection, MRB review, and package and shipping inspection.

Client: Baker Hughes
Product in GFDS System
Vendor: Himile Mechanical Manufacturing Co. Ltd.
Product: Porch, Termination, Male Hub/pup-piece
Position: Inspector
Inspected raw materials and machining.
Inspected NDT before clad welding and monitored clad welding.
Inspected clad welding, including PMI, CRA thickness, and NDT.
Performed dimensional inspection and witnessed hydrostatic and gas tests.
Inspected blasting, painting, assembly, adhesion, and holiday testing.
Witnessed FAT, including weight, visual, electrical continuity, and back seal tests.
Performed final inspection, MRB review, and package and shipping inspection.

Pipe & tube
Product: API 5L SMLS & welded pipes, 5D inducted bends, Stainless Steel SMLS & Welded tubes, Nickel Alloy pipes, Square & Rectangular tube, Cu Alloy SMLS pipes
Standards: API 5L, EN 10216-3, KOC-MS-002 PT.1, ASTM B423, MSS SP-75-2008, ASTM A312
Position: Third party inspection & Certification
Performed manufacturing procedure qualification testing.
Inspected product chemical analysis and mechanical property testing.
Witnessed hydrostatic and NDT testing, including ET, UT, RT, and MT.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: KOC, Ruicheng, PANTECH CORPORATION SDA BHD
Pipe fittings
Vendor: Zhejiang Jiuli Hi-Tech Metals, Shanghai Shihang Copper Nickel Fittings, Shanghai Feiting pipe Manufacture, Shanxi ST&H, Luda (Taian) Industry
Product: ASTM Blind flange, Flange, Reducer, Tee, Elbow, Weldolet, Coupling, Thread End Cap, Sockolet, Nipple,etc
Standards: ASME B16.5 ASME B16.9, ASME B16.11, MSS SP-97
Position: Third party inspection & Certification
Reviewed documents.
Inspected chemical analysis and mechanical property testing.
Witnessed hardness and PMI tests.
Performed dimensional and visual quality inspection.
Inspected packing, marking, and coating.

Client: Neway Valve Plant, O& G Engineering, KOGAS, Rotary Engneering
Valve
Product: Ball Valve, Plug Valve, Gate Valve, Control Valve
Standards: API 6D, ASME B16.34, API 598
Position: Third party inspection & Certification
Reviewed documents.
Witnessed PMI, mechanical property, hardness, and NDT testing, including PT, MT, UT, and RT.
Performed assembly, visual, and dimensional inspection.
Witnessed hydraulic pressure, shell, seat, backseat, low-pressure gas, and operation tests.
Inspected painting, marking, and packing.

Client: Oil and Natural Gas Corporation
SubSurface Safety Valve & Packer
Vendor: Schlumberger Reservoir, Chuannan Energy technology
Product: SubSurface Safety Valve & Packer
Standards: API 14A, API 11D
Position: Third party inspection & Certification
Reviewed documents.
Witnessed drift and function tests.
Performed dimensional, visual, marking, and coating and protection inspection.

Client: Jiangyin Xingcheng, Howco, Hama, Shangdong Iron and Steel, Baoshan Iron & Steel, Leongjin (Jintan), Laiwu Company of Shandong Iron and steel; Jiangnan Boiler & pressure vessel
Steel plates and forging
Product: Shipped steel plates, Spheroidal Graphite Cast Iron, AISI 4130, 8630 forging, low alloy steel
Standards: AISI 4130 & 8630, GB 712, EN 10025-1~6, EN 10210-1, EN 10297-1, EN10216-3 & DIN 2448, B/T 1348, ABS rules, ASME SA336
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed hardness, UT, and MT tests.
Performed visual and dimensional inspection.
Inspected painting, marking, and packing.

Client: Shanghai Baoling, Laiwu Steel Group Zibo Anchor Chain, Tengzhou Chenjin, Changshu Haihong Ship Equipment, Jiangsu Xiangsheng, Jianfeng Sling
Chain
Product: Mooring Chain Cable, Wire rope Sling, Tonsberg Mooring Links & Mandal Fairlead Shackle, Chain Grapnel & J hook, Pear Links
Position: Third party inspection & Certification
Reviewed documents.
Witnessed chemical analysis and mechanical property testing.
Witnessed proof-load and break-load tests.
Performed dimensional and visual quality inspection.

Client: Taicang Kaide
Anodes
Product: Al Anode, Zn Anode
Position: Third party inspection & Certification
Reviewed documents.
Monitored casing.
Witnessed chemical and electrochemical analysis.
Performed cross-cut, resistance, weight, dimensional, and visual quality inspection.

Client: Kade Heavy, Star Rubber, Qingdao Shunshine, Qingdao Dongwo, Shanghai sailfish Rope, Shandong Rope Technology
Other products
Product: Electric heater Core, Life raft, Pick Up Buoys, Anchor Buoys, Polyamide (Nylone) 8-strand ropes
Position: Third party inspection & Certification
Reviewed documents.
Witnessed hydrostatic, performance, and break-load tests.
Performed dimensional and visual quality inspection.

Client: Seacube, CAI, Seaco, CIMC(Ningbo)
Construction of Container
Vendor: Ningbo Xinhuachang, NCLE, Ningbo Pacific
Product: Containers
Position: Inspector
Reviewed documents.
Inspected floorboards and corner-fitting sampling.
Witnessed relative testing.
Inspected welding, assembly, routing, and dimensions.
Performed visual quality inspection after welding.
Performed coating inspection.
Witnessed general prototype testing and whole-container inspection.

Client: NP QHG port, PSA CORPORATION LTD, MEPT, VOLTRITERMIANAL EUROPA S.p.A, Ningbo Daxie, Ningbo Yuandong, Ningbo Port Import & Export, PSA PANAMA INTERNATIONAL, TERMINAL S.A (PPIT), Zhenjiang West
Construction of Heavy lifting Equipment
Product: Container Cranes (RTG/STS), Offshore Crane & Hydraulic Slewing Crane
Position: Inspector
Reviewed related documents and procedures, including WPS, welder qualification, and drawings.
Performed raw material re-inspection.
Inspected main structural steel assembly.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Performed structural final inspection and coating inspection.
Witnessed FAT and EFAT of cranes.

Steel bridge (Peru bridge, America New San Francisco Oakland Bay Bridge, Taizhou Bridge, Sutong Bridge)
Product: Steel bridge
Position: CWI inspector
Performed raw material re-inspection.
Witnessed mechanical property testing and product chemical analysis for steel plates, bolts, and nuts.
Witnessed welding procedure qualification and welder qualification tests.
Inspected pre-welding and welding processes.
Performed visual quality inspection after welding.
Checked zinc coating of fabricated products.

Client: SAMSUNG ENGINEERING CO., LTD, Hangzhou Steam Turbine Co., Ltd, Himile Mechanical Manufacturing
Construction of Equipment
Product: Gland Condenser & Handing Clamp
Position: Inspector
Reviewed quality-control documents, including ITP, WPS/PQR, WQT, and NDT.
Reviewed material, equipment calibration, and consumable certificates.
Witnessed hydrostatic testing and cleaning and dry checks.
Witnessed surface preparation and performed visual and dry-film checks.
Inspected rust prevention, including VCI application inside the gland condenser.
Performed visual and dimensional inspection, including nameplates.
Inspected packing and marking.
Reviewed manufacturing final inspection.

LANGUAGES
English (speaking, reading, writing, listening)
Chinese (Native language)

SKILLS
Material Inspection
Steel Structure Inspection
Welding Inspection
Pressure Vessel Inspection
FPSO Topside Inspection
Subsea Product Inspection
Crane and Heavy Lifting Equipment Inspection
Third-Party Inspection and Certification
Coating Inspection
Mechanical Inspection
Package and Skid Inspection
Vendor Inspection
Quality Document Review
NDT Inspection
Client and Contractor Coordination

COMMODITIES
Coating
Pressure Vessels
FPSO Packages
Subsea Products
Steel Structures
Pipes and Tubes
Piping Fittings
Valves
Chains
Bridges
Steel Plates
Forgings
Gas Turbine Cylinders
Pumps
Skids
Separators
Scrubbers
Exchangers
Cranes
Containers
Anodes
Wire Rope Slings
Life Rafts
Buoys
Ropes

fulkrum.com

image2.png
\




image200.png
\




